,Mounting##Other##,Output##Other##,Housing Type##OTHER##,"CRI, CCT##Other##",Beam Spread##OTHER##,Model##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Voltage Comment##OTHER##,Photometric Web File##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Instruction Sheet Link##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,C Housing##OTHER##,C High Output##Other##,C Low Output##Other##,C Flanged##OTHER##
E3RLF-LH8270AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RLF-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8270AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RLF-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8270ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RLF-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8270ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RLF-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8271AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RLF-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8271AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RLF-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8271ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RLF-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8271ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RLF-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8272AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RLF-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8272AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RLF-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8272ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RLF-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8272ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RLF-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8274AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RLF-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8274AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RLF-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8274ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RLF-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8274ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RLF-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8276AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RLF-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8276AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RLF-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8276ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RLF-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8276ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RLF-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8300AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RLF-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8300AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RLF-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8300ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RLF-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8300ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RLF-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8301AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RLF-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8301AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RLF-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8301ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RLF-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8301ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RLF-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8302AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RLF-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8302AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RLF-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8302ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RLF-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8302ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RLF-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8304AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RLF-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8304AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RLF-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8304ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RLF-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8304ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RLF-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8306AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RLF-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8306AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RLF-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8306ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RLF-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8306ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RLF-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8350AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RLF-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8350AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RLF-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8350ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RLF-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8350ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RLF-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8351AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RLF-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8351AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RLF-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8351ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RLF-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8351ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RLF-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8352AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RLF-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8352AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RLF-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8352ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RLF-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8352ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RLF-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8354AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RLF-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8354AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RLF-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8354ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RLF-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8354ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RLF-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8356AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RLF-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8356AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RLF-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8356ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RLF-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH8356ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RLF-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RLF-LH9270AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RLF-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9270AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RLF-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9270ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RLF-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9270ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RLF-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9271AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RLF-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9271AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RLF-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9271ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RLF-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9271ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RLF-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9272AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RLF-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9272AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RLF-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9272ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RLF-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9272ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RLF-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9274AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RLF-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9274AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RLF-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9274ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RLF-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9274ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RLF-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9276AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RLF-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9276AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RLF-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9276ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RLF-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9276ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RLF-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9300AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RLF-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9300AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RLF-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9300ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RLF-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9300ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RLF-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9301AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RLF-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9301AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RLF-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9301ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RLF-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9301ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RLF-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9302AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RLF-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9302AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RLF-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9302ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RLF-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9302ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RLF-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9304AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RLF-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9304AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RLF-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9304ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RLF-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9304ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RLF-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9306AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RLF-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9306AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RLF-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9306ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RLF-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9306ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RLF-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9350AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RLF-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9350AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RLF-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9350ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RLF-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9350ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RLF-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9351AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RLF-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9351AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RLF-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9351ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RLF-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9351ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RLF-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9352AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RLF-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9352AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RLF-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9352ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RLF-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9352ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RLF-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9354AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RLF-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9354AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RLF-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9354ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RLF-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9354ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RLF-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9356AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RLF-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9356AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RLF-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9356ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RLF-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LH9356ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RLF-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RLF-LHWD0AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD0AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD0ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD0ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD1AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD1AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD1ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD1ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD2AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD2AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD2ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD2ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD4AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD4AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD4ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD4ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD6AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD6AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD6ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LHWD6ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RLF-LO8270AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RLF-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8270AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RLF-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8270ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RLF-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8270ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RLF-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8271AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RLF-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8271AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RLF-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8271ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RLF-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8271ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RLF-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8272AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RLF-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8272AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RLF-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8272ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RLF-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8272ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RLF-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8274AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RLF-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8274AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RLF-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8274ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RLF-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8274ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RLF-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8276AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RLF-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8276AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RLF-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8276ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RLF-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8276ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RLF-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8300AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RLF-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8300AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RLF-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8300ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RLF-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8300ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RLF-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8301AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RLF-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8301AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RLF-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8301ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RLF-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8301ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RLF-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8302AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RLF-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8302AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RLF-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8302ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RLF-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8302ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RLF-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8304AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RLF-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8304AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RLF-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8304ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RLF-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8304ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RLF-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8306AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RLF-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8306AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RLF-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8306ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RLF-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8306ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RLF-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8350AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RLF-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8350AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RLF-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8350ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RLF-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8350ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RLF-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8351AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RLF-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8351AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RLF-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8351ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RLF-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8351ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RLF-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8352AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RLF-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8352AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RLF-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8352ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RLF-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8352ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RLF-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8354AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RLF-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8354AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RLF-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8354ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RLF-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8354ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RLF-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8356AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RLF-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8356AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RLF-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8356ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RLF-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO8356ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RLF-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RLF-LO9270AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RLF-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9270AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RLF-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9270ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RLF-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9270ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RLF-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9271AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RLF-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9271AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RLF-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9271ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RLF-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9271ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RLF-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9272AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RLF-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9272AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RLF-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9272ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RLF-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9272ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RLF-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9274AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RLF-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9274AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RLF-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9274ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RLF-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9274ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RLF-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9276AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RLF-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9276AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RLF-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9276ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RLF-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9276ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RLF-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9300AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RLF-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9300AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RLF-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9300ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RLF-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9300ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RLF-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9301AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RLF-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9301AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RLF-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9301ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RLF-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9301ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RLF-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9302AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RLF-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9302AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RLF-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9302ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RLF-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9302ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RLF-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9304AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RLF-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9304AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RLF-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9304ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RLF-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9304ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RLF-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9306AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RLF-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9306AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RLF-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9306ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RLF-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9306ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RLF-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9350AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RLF-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9350AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RLF-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9350ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RLF-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9350ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RLF-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9351AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RLF-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9351AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RLF-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9351ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RLF-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9351ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RLF-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9352AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RLF-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9352AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RLF-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9352ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RLF-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9352ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RLF-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9354AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RLF-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9354AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RLF-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9354ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RLF-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9354ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RLF-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9356AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RLF-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9356AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RLF-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9356ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RLF-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LO9356ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RLF-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RLF-LOWD0AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD0AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD0ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD0ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RLF-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD1AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD1AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD1ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD1ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RLF-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD2AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD2AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD2ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD2ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RLF-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD4AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD4AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD4ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD4ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RLF-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD6AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD6AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD6ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RLF-LOWD6ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RLF-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RFF-LH8270AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RFF-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8270AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RFF-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8270ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RFF-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8270ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RFF-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8271AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RFF-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8271AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RFF-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8271ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RFF-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8271ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RFF-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8272AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RFF-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8272AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RFF-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8272ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RFF-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8272ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RFF-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8274AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RFF-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8274AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RFF-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8274ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RFF-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8274ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RFF-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8276AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RFF-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8276AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RFF-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8276ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RFF-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8276ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RFF-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8300AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RFF-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8300AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RFF-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8300ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RFF-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8300ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RFF-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8301AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RFF-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8301AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RFF-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8301ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RFF-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8301ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RFF-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8302AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RFF-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8302AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RFF-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8302ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RFF-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8302ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RFF-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8304AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RFF-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8304AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RFF-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8304ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RFF-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8304ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RFF-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8306AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RFF-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8306AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RFF-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8306ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RFF-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8306ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RFF-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8350AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RFF-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8350AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RFF-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8350ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RFF-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8350ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RFF-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8351AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RFF-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8351AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RFF-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8351ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RFF-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8351ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RFF-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8352AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RFF-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8352AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RFF-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8352ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RFF-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8352ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RFF-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8354AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RFF-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8354AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RFF-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8354ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RFF-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8354ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RFF-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8356AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RFF-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8356AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RFF-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8356ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RFF-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH8356ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RFF-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,1
E3RFF-LH9270AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RFF-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9270AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RFF-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9270ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RFF-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9270ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RFF-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9271AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RFF-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9271AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RFF-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9271ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RFF-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9271ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RFF-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9272AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RFF-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9272AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RFF-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9272ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RFF-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9272ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RFF-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9274AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RFF-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9274AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RFF-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9274ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RFF-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9274ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RFF-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9276AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RFF-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9276AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RFF-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9276ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RFF-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9276ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RFF-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9300AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RFF-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9300AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RFF-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9300ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RFF-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9300ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RFF-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9301AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RFF-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9301AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RFF-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9301ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RFF-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9301ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RFF-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9302AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RFF-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9302AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RFF-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9302ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RFF-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9302ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RFF-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9304AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RFF-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9304AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RFF-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9304ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RFF-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9304ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RFF-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9306AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RFF-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9306AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RFF-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9306ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RFF-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9306ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RFF-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9350AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RFF-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9350AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RFF-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9350ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RFF-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9350ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RFF-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9351AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RFF-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9351AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RFF-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9351ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RFF-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9351ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RFF-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9352AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RFF-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9352AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RFF-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9352ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RFF-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9352ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RFF-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9354AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RFF-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9354AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RFF-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9354ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RFF-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9354ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RFF-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9356AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RFF-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9356AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RFF-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9356ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RFF-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LH9356ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RFF-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,1
E3RFF-LHWD0AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD0AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD0ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD0ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD1AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD1AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD1ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD1ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD2AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD2AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD2ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD2ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD4AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD4AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD4ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD4ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD6AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD6AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD6ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LHWD6ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,1
E3RFF-LO8270AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RFF-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8270AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RFF-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8270ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RFF-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8270ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RFF-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8271AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RFF-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8271AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RFF-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8271ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RFF-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8271ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RFF-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8272AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RFF-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8272AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RFF-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8272ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RFF-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8272ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RFF-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8274AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RFF-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8274AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RFF-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8274ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RFF-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8274ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RFF-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8276AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RFF-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8276AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RFF-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8276ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RFF-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8276ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RFF-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8300AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RFF-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8300AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RFF-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8300ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RFF-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8300ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RFF-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8301AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RFF-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8301AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RFF-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8301ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RFF-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8301ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RFF-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8302AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RFF-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8302AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RFF-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8302ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RFF-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8302ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RFF-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8304AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RFF-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8304AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RFF-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8304ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RFF-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8304ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RFF-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8306AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RFF-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8306AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RFF-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8306ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RFF-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8306ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RFF-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8350AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RFF-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8350AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RFF-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8350ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RFF-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8350ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RFF-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8351AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RFF-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8351AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RFF-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8351ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RFF-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8351ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RFF-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8352AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RFF-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8352AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RFF-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8352ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RFF-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8352ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RFF-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8354AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RFF-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8354AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RFF-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8354ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RFF-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8354ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RFF-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8356AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RFF-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8356AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RFF-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8356ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RFF-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO8356ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RFF-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,1
E3RFF-LO9270AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RFF-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9270AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RFF-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9270ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RFF-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9270ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RFF-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9271AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RFF-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9271AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RFF-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9271ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RFF-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9271ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RFF-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9272AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RFF-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9272AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RFF-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9272ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RFF-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9272ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RFF-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9274AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RFF-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9274AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RFF-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9274ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RFF-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9274ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RFF-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9276AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RFF-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9276AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RFF-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9276ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RFF-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9276ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RFF-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9300AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RFF-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9300AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RFF-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9300ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RFF-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9300ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RFF-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9301AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RFF-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9301AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RFF-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9301ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RFF-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9301ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RFF-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9302AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RFF-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9302AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RFF-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9302ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RFF-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9302ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RFF-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9304AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RFF-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9304AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RFF-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9304ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RFF-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9304ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RFF-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9306AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RFF-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9306AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RFF-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9306ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RFF-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9306ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RFF-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9350AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RFF-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9350AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RFF-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9350ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RFF-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9350ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RFF-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9351AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RFF-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9351AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RFF-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9351ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RFF-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9351ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RFF-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9352AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RFF-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9352AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RFF-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9352ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RFF-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9352ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RFF-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9354AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RFF-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9354AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RFF-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9354ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RFF-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9354ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RFF-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9356AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RFF-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9356AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RFF-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9356ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RFF-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LO9356ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RFF-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,1
E3RFF-LOWD0AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD0AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD0ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD0ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RFF-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD1AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD1AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD1ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD1ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RFF-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD2AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD2AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD2ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD2ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RFF-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD4AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD4AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD4ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD4ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RFF-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD6AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD6AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD6ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RFF-LOWD6ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RFF-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,1
E3RWC-LH8270AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RWC-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8270AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RWC-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8270ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RWC-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8270ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RWC-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8271AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RWC-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8271AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RWC-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8271ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RWC-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8271ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RWC-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8272AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RWC-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8272AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RWC-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8272ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RWC-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8272ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RWC-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8274AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RWC-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8274AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RWC-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8274ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RWC-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8274ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RWC-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8276AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RWC-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8276AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RWC-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8276ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RWC-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8276ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RWC-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8300AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RWC-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8300AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RWC-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8300ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RWC-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8300ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RWC-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8301AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RWC-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8301AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RWC-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8301ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RWC-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8301ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RWC-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8302AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RWC-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8302AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RWC-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8302ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RWC-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8302ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RWC-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8304AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RWC-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8304AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RWC-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8304ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RWC-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8304ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RWC-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8306AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RWC-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8306AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RWC-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8306ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RWC-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8306ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RWC-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8350AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RWC-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8350AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RWC-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8350ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RWC-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8350ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RWC-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8351AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RWC-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8351AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RWC-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8351ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RWC-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8351ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RWC-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8352AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RWC-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8352AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RWC-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8352ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RWC-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8352ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RWC-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8354AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RWC-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8354AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RWC-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8354ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RWC-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8354ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RWC-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8356AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RWC-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8356AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RWC-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8356ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RWC-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH8356ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RWC-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,1,1,0,0
E3RWC-LH9270AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RWC-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9270AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RWC-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9270ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RWC-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9270ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RWC-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9271AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RWC-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9271AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RWC-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9271ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RWC-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9271ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RWC-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9272AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RWC-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9272AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RWC-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9272ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RWC-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9272ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RWC-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9274AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RWC-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9274AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RWC-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9274ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RWC-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9274ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RWC-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9276AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RWC-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9276AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RWC-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9276ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RWC-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9276ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RWC-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9300AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RWC-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9300AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RWC-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9300ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RWC-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9300ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RWC-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9301AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RWC-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9301AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RWC-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9301ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RWC-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9301ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RWC-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9302AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RWC-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9302AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RWC-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9302ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RWC-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9302ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RWC-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9304AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RWC-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9304AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RWC-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9304ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RWC-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9304ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RWC-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9306AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RWC-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9306AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RWC-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9306ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RWC-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9306ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RWC-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9350AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RWC-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9350AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RWC-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9350ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RWC-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9350ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RWC-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9351AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RWC-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9351AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RWC-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9351ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RWC-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9351ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RWC-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9352AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RWC-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9352AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RWC-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9352ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RWC-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9352ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RWC-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9354AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RWC-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9354AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RWC-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9354ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RWC-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9354ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RWC-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9356AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RWC-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9356AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RWC-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9356ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RWC-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LH9356ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RWC-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,1,1,0,0
E3RWC-LHWD0AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD0AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD0ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD0ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD1AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD1AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD1ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD1ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD2AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD2AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD2ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD2ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD4AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD4AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD4ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD4ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD6AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD6AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD6ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LHWD6ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,1,1,0,0
E3RWC-LO8270AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RWC-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8270AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3RWC-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8270ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RWC-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8270ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3RWC-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8271AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RWC-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8271AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3RWC-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8271ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RWC-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8271ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3RWC-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8272AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RWC-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8272AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3RWC-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8272ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RWC-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8272ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3RWC-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8274AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RWC-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8274AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3RWC-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8274ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RWC-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8274ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3RWC-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8276AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RWC-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8276AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3RWC-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8276ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RWC-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8276ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3RWC-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8300AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RWC-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8300AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3RWC-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8300ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RWC-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8300ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3RWC-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8301AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RWC-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8301AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3RWC-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8301ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RWC-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8301ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3RWC-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8302AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RWC-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8302AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3RWC-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8302ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RWC-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8302ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3RWC-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8304AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RWC-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8304AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3RWC-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8304ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RWC-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8304ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3RWC-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8306AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RWC-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8306AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3RWC-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8306ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RWC-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8306ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3RWC-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8350AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RWC-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8350AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3RWC-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8350ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RWC-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8350ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3RWC-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8351AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RWC-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8351AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3RWC-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8351ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RWC-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8351ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3RWC-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8352AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RWC-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8352AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3RWC-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8352ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RWC-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8352ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3RWC-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8354AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RWC-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8354AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3RWC-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8354ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RWC-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8354ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3RWC-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8356AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RWC-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8356AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3RWC-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8356ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RWC-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO8356ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3RWC-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,1,0,1,0
E3RWC-LO9270AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RWC-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9270AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3RWC-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9270ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RWC-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9270ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3RWC-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9271AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RWC-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9271AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3RWC-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9271ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RWC-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9271ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3RWC-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9272AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RWC-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9272AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3RWC-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9272ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RWC-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9272ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3RWC-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9274AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RWC-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9274AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3RWC-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9274ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RWC-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9274ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3RWC-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9276AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RWC-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9276AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3RWC-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9276ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RWC-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9276ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3RWC-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9300AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RWC-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9300AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3RWC-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9300ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RWC-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9300ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3RWC-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9301AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RWC-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9301AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3RWC-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9301ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RWC-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9301ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3RWC-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9302AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RWC-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9302AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3RWC-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9302ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RWC-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9302ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3RWC-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9304AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RWC-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9304AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3RWC-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9304ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RWC-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9304ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3RWC-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9306AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RWC-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9306AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3RWC-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9306ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RWC-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9306ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3RWC-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9350AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RWC-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9350AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3RWC-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9350ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RWC-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9350ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3RWC-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9351AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RWC-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9351AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3RWC-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9351ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RWC-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9351ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3RWC-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9352AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RWC-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9352AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3RWC-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9352ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RWC-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9352ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3RWC-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9354AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RWC-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9354AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3RWC-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9354ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RWC-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9354ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3RWC-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9356AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RWC-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9356AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3RWC-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9356ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RWC-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LO9356ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3RWC-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,1,0,1,0
E3RWC-LOWD0AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD0AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD0ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD0ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3RWC-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD1AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD1AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD1ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD1ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3RWC-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD2AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD2AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD2ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD2ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3RWC-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD4AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD4AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD4ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD4ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3RWC-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD6AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD6AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD6ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3RWC-LOWD6ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3RWC-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,1,0,1,0
E3SLF-LH8270AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SLF-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8270AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SLF-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8270ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SLF-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8270ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SLF-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8271AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SLF-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8271AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SLF-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8271ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SLF-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8271ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SLF-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8272AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SLF-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8272AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SLF-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8272ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SLF-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8272ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SLF-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8274AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SLF-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8274AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SLF-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8274ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SLF-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8274ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SLF-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8276AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SLF-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8276AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SLF-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8276ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SLF-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8276ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SLF-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8300AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SLF-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8300AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SLF-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8300ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SLF-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8300ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SLF-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8301AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SLF-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8301AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SLF-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8301ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SLF-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8301ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SLF-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8302AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SLF-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8302AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SLF-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8302ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SLF-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8302ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SLF-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8304AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SLF-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8304AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SLF-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8304ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SLF-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8304ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SLF-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8306AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SLF-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8306AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SLF-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8306ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SLF-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8306ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SLF-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8350AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SLF-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8350AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SLF-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8350ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SLF-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8350ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SLF-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8351AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SLF-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8351AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SLF-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8351ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SLF-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8351ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SLF-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8352AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SLF-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8352AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SLF-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8352ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SLF-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8352ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SLF-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8354AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SLF-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8354AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SLF-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8354ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SLF-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8354ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SLF-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8356AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SLF-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8356AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SLF-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8356ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SLF-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH8356ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SLF-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SLF-LH9270AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SLF-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9270AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SLF-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9270ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SLF-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9270ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SLF-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9271AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SLF-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9271AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SLF-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9271ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SLF-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9271ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SLF-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9272AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SLF-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9272AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SLF-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9272ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SLF-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9272ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SLF-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9274AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SLF-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9274AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SLF-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9274ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SLF-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9274ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SLF-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9276AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SLF-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9276AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SLF-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9276ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SLF-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9276ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SLF-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9300AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SLF-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9300AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SLF-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9300ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SLF-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9300ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SLF-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9301AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SLF-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9301AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SLF-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9301ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SLF-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9301ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SLF-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9302AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SLF-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9302AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SLF-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9302ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SLF-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9302ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SLF-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9304AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SLF-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9304AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SLF-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9304ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SLF-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9304ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SLF-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9306AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SLF-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9306AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SLF-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9306ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SLF-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9306ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SLF-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9350AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SLF-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9350AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SLF-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9350ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SLF-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9350ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SLF-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9351AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SLF-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9351AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SLF-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9351ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SLF-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9351ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SLF-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9352AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SLF-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9352AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SLF-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9352ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SLF-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9352ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SLF-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9354AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SLF-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9354AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SLF-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9354ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SLF-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9354ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SLF-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9356AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SLF-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9356AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SLF-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9356ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SLF-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LH9356ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SLF-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SLF-LHWD0AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD0AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD0ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD0ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD1AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD1AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD1ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD1ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD2AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD2AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD2ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD2ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD4AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD4AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD4ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD4ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD6AS_,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD6AS-277,Flangeless,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD6ACS_,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LHWD6ACS-277,Flangeless,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SLF-LO8270AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SLF-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8270AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SLF-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8270ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SLF-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8270ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SLF-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8271AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SLF-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8271AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SLF-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8271ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SLF-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8271ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SLF-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8272AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SLF-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8272AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SLF-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8272ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SLF-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8272ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SLF-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8274AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SLF-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8274AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SLF-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8274ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SLF-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8274ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SLF-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8276AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SLF-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8276AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SLF-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8276ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SLF-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8276ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SLF-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8300AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SLF-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8300AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SLF-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8300ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SLF-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8300ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SLF-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8301AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SLF-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8301AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SLF-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8301ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SLF-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8301ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SLF-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8302AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SLF-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8302AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SLF-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8302ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SLF-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8302ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SLF-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8304AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SLF-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8304AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SLF-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8304ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SLF-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8304ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SLF-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8306AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SLF-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8306AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SLF-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8306ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SLF-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8306ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SLF-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8350AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SLF-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8350AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SLF-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8350ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SLF-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8350ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SLF-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8351AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SLF-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8351AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SLF-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8351ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SLF-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8351ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SLF-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8352AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SLF-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8352AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SLF-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8352ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SLF-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8352ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SLF-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8354AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SLF-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8354AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SLF-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8354ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SLF-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8354ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SLF-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8356AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SLF-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8356AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SLF-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8356ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SLF-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO8356ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SLF-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SLF-LO9270AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SLF-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9270AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SLF-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9270ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SLF-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9270ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SLF-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9271AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SLF-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9271AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SLF-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9271ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SLF-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9271ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SLF-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9272AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SLF-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9272AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SLF-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9272ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SLF-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9272ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SLF-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9274AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SLF-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9274AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SLF-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9274ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SLF-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9274ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SLF-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9276AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SLF-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9276AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SLF-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9276ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SLF-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9276ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SLF-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9300AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SLF-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9300AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SLF-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9300ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SLF-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9300ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SLF-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9301AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SLF-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9301AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SLF-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9301ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SLF-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9301ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SLF-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9302AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SLF-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9302AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SLF-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9302ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SLF-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9302ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SLF-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9304AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SLF-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9304AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SLF-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9304ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SLF-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9304ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SLF-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9306AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SLF-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9306AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SLF-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9306ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SLF-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9306ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SLF-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9350AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SLF-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9350AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SLF-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9350ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SLF-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9350ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SLF-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9351AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SLF-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9351AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SLF-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9351ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SLF-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9351ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SLF-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9352AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SLF-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9352AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SLF-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9352ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SLF-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9352ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SLF-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9354AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SLF-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9354AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SLF-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9354ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SLF-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9354ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SLF-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9356AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SLF-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9356AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SLF-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9356ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SLF-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LO9356ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SLF-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SLF-LOWD0AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD0AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD0ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD0ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SLF-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD1AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD1AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD1ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD1ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SLF-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD2AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD2AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD2ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD2ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SLF-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD4AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD4AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD4ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD4ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SLF-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD6AS_,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD6AS-277,Flangeless,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD6ACS_,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SLF-LOWD6ACS-277,Flangeless,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SLF-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SFF-LH8270AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SFF-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8270AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SFF-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8270ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SFF-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8270ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SFF-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8271AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SFF-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8271AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SFF-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8271ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SFF-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8271ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SFF-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8272AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SFF-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8272AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SFF-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8272ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SFF-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8272ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SFF-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8274AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SFF-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8274AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SFF-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8274ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SFF-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8274ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SFF-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8276AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SFF-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8276AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SFF-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8276ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SFF-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8276ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SFF-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8300AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SFF-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8300AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SFF-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8300ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SFF-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8300ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SFF-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8301AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SFF-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8301AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SFF-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8301ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SFF-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8301ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SFF-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8302AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SFF-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8302AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SFF-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8302ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SFF-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8302ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SFF-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8304AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SFF-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8304AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SFF-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8304ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SFF-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8304ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SFF-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8306AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SFF-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8306AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SFF-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8306ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SFF-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8306ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SFF-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8350AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SFF-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8350AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SFF-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8350ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SFF-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8350ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SFF-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8351AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SFF-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8351AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SFF-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8351ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SFF-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8351ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SFF-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8352AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SFF-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8352AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SFF-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8352ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SFF-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8352ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SFF-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8354AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SFF-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8354AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SFF-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8354ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SFF-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8354ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SFF-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8356AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SFF-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8356AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SFF-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8356ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SFF-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH8356ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SFF-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,1
E3SFF-LH9270AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SFF-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9270AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SFF-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9270ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SFF-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9270ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SFF-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9271AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SFF-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9271AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SFF-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9271ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SFF-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9271ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SFF-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9272AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SFF-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9272AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SFF-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9272ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SFF-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9272ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SFF-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9274AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SFF-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9274AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SFF-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9274ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SFF-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9274ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SFF-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9276AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SFF-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9276AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SFF-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9276ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SFF-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9276ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SFF-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9300AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SFF-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9300AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SFF-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9300ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SFF-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9300ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SFF-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9301AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SFF-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9301AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SFF-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9301ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SFF-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9301ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SFF-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9302AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SFF-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9302AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SFF-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9302ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SFF-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9302ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SFF-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9304AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SFF-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9304AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SFF-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9304ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SFF-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9304ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SFF-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9306AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SFF-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9306AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SFF-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9306ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SFF-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9306ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SFF-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9350AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SFF-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9350AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SFF-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9350ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SFF-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9350ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SFF-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9351AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SFF-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9351AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SFF-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9351ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SFF-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9351ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SFF-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9352AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SFF-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9352AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SFF-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9352ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SFF-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9352ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SFF-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9354AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SFF-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9354AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SFF-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9354ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SFF-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9354ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SFF-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9356AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SFF-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9356AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SFF-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9356ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SFF-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LH9356ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SFF-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,1
E3SFF-LHWD0AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD0AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD0ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD0ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD1AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD1AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD1ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD1ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD2AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD2AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD2ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD2ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD4AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD4AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD4ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD4ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD6AS_,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD6AS-277,Flanged,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD6ACS_,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LHWD6ACS-277,Flanged,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,1
E3SFF-LO8270AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SFF-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8270AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SFF-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8270ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SFF-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8270ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SFF-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8271AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SFF-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8271AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SFF-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8271ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SFF-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8271ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SFF-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8272AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SFF-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8272AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SFF-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8272ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SFF-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8272ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SFF-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8274AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SFF-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8274AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SFF-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8274ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SFF-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8274ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SFF-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8276AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SFF-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8276AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SFF-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8276ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SFF-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8276ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SFF-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8300AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SFF-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8300AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SFF-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8300ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SFF-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8300ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SFF-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8301AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SFF-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8301AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SFF-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8301ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SFF-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8301ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SFF-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8302AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SFF-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8302AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SFF-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8302ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SFF-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8302ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SFF-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8304AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SFF-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8304AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SFF-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8304ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SFF-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8304ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SFF-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8306AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SFF-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8306AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SFF-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8306ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SFF-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8306ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SFF-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8350AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SFF-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8350AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SFF-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8350ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SFF-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8350ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SFF-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8351AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SFF-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8351AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SFF-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8351ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SFF-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8351ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SFF-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8352AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SFF-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8352AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SFF-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8352ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SFF-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8352ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SFF-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8354AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SFF-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8354AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SFF-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8354ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SFF-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8354ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SFF-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8356AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SFF-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8356AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SFF-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8356ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SFF-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO8356ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SFF-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,1
E3SFF-LO9270AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SFF-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9270AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SFF-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9270ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SFF-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9270ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SFF-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9271AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SFF-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9271AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SFF-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9271ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SFF-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9271ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SFF-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9272AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SFF-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9272AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SFF-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9272ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SFF-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9272ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SFF-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9274AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SFF-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9274AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SFF-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9274ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SFF-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9274ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SFF-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9276AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SFF-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9276AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SFF-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9276ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SFF-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9276ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SFF-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9300AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SFF-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9300AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SFF-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9300ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SFF-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9300ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SFF-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9301AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SFF-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9301AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SFF-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9301ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SFF-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9301ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SFF-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9302AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SFF-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9302AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SFF-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9302ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SFF-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9302ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SFF-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9304AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SFF-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9304AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SFF-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9304ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SFF-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9304ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SFF-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9306AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SFF-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9306AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SFF-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9306ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SFF-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9306ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SFF-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9350AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SFF-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9350AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SFF-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9350ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SFF-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9350ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SFF-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9351AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SFF-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9351AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SFF-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9351ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SFF-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9351ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SFF-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9352AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SFF-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9352AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SFF-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9352ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SFF-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9352ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SFF-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9354AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SFF-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9354AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SFF-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9354ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SFF-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9354ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SFF-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9356AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SFF-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9356AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SFF-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9356ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SFF-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LO9356ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SFF-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,1
E3SFF-LOWD0AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD0AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD0ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD0ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SFF-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD1AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD1AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD1ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD1ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SFF-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD2AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD2AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD2ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD2ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SFF-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD4AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD4AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD4ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD4ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SFF-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD6AS_,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD6AS-277,Flanged,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD6ACS_,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SFF-LOWD6ACS-277,Flanged,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SFF-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,1
E3SWC-LH8270AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SWC-LH8270AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8270AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SWC-LH8270AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8270ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SWC-LH8270ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8270ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SWC-LH8270ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8271AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SWC-LH8271AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8271AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SWC-LH8271AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8271ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SWC-LH8271ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8271ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SWC-LH8271ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8272AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SWC-LH8272AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8272AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SWC-LH8272AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8272ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SWC-LH8272ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8272ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SWC-LH8272ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8274AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SWC-LH8274AS_,17,17 Watts,1800,2700,120,120 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8274AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SWC-LH8274AS-277,17,17 Watts,1800,2700,277,277 Volt,103017649CHI-034 GB E3SFF-LH8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8274ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SWC-LH8274ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8274ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SWC-LH8274ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8276AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SWC-LH8276AS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8276AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SWC-LH8276AS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8276ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SWC-LH8276ACS_,17,17 Watts,1800,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8276ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SWC-LH8276ACS-277,17,17 Watts,1800,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8300AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SWC-LH8300AS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8300AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SWC-LH8300AS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8300ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SWC-LH8300ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8300ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SWC-LH8300ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8301AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SWC-LH8301AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8301AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SWC-LH8301AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-030 GB E3SFF-LH8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8301ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SWC-LH8301ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8301ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SWC-LH8301ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8302AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SWC-LH8302AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8302AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SWC-LH8302AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-026 GB E3SFF-LH8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8302ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SWC-LH8302ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8302ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SWC-LH8302ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8304AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SWC-LH8304AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8304AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SWC-LH8304AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-022 GB E3SFF-LH8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8304ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SWC-LH8304ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8304ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SWC-LH8304ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8306AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SWC-LH8306AS_,17,17 Watts,1800,3000,120,120 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8306AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SWC-LH8306AS-277,17,17 Watts,1800,3000,277,277 Volt,103017649CHI-091 GB E3SFF-LH8306AI.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8306ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SWC-LH8306ACS_,17,17 Watts,1800,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8306ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SWC-LH8306ACS-277,17,17 Watts,1800,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8350AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SWC-LH8350AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8350AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SWC-LH8350AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8350ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SWC-LH8350ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8350ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SWC-LH8350ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8351AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SWC-LH8351AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8351AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SWC-LH8351AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8351ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SWC-LH8351ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8351ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SWC-LH8351ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8352AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SWC-LH8352AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8352AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SWC-LH8352AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8352ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SWC-LH8352ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8352ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SWC-LH8352ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8354AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SWC-LH8354AS_,17,17 Watts,1800,3500,120,120 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8354AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SWC-LH8354AS-277,17,17 Watts,1800,3500,277,277 Volt,103017649CHI-038 GB E3SFF-LH8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8354ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SWC-LH8354ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8354ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SWC-LH8354ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8356AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SWC-LH8356AS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8356AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SWC-LH8356AS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8356ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SWC-LH8356ACS_,17,17 Watts,1800,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH8356ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SWC-LH8356ACS-277,17,17 Watts,1800,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,106,17,3,1,0,0
E3SWC-LH9270AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SWC-LH9270AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9270AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SWC-LH9270AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9270ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SWC-LH9270ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9270ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SWC-LH9270ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9271AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SWC-LH9271AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9271AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SWC-LH9271AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9271ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SWC-LH9271ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9271ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SWC-LH9271ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9272AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SWC-LH9272AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9272AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SWC-LH9272AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9272ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SWC-LH9272ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9272ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SWC-LH9272ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9274AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SWC-LH9274AS_,17,17 Watts,1450,2700,120,120 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9274AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SWC-LH9274AS-277,17,17 Watts,1450,2700,277,277 Volt,103017649CHI-036 GB E3SFF-LH9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9274ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SWC-LH9274ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9274ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SWC-LH9274ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9276AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SWC-LH9276AS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9276AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SWC-LH9276AS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9276ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SWC-LH9276ACS_,17,17 Watts,1450,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9276ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SWC-LH9276ACS-277,17,17 Watts,1450,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9300AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SWC-LH9300AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9300AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SWC-LH9300AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-045 GB E3SRF-LH9300DN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9300ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SWC-LH9300ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9300ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SWC-LH9300ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9301AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SWC-LH9301AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9301AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SWC-LH9301AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-032 GB E3SFF-LH9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9301ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SWC-LH9301ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9301ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SWC-LH9301ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9302AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SWC-LH9302AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9302AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SWC-LH9302AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-028 GB E3SFF-LH9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9302ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SWC-LH9302ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9302ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SWC-LH9302ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9304AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SWC-LH9304AS_,17,17 Watts,1450,3000,120,120 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9304AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SWC-LH9304AS-277,17,17 Watts,1450,3000,277,277 Volt,103017649CHI-024 GB E3SFF-LH9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9304ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SWC-LH9304ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9304ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SWC-LH9304ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9306AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SWC-LH9306AS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9306AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SWC-LH9306AS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9306ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SWC-LH9306ACS_,17,17 Watts,1450,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9306ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SWC-LH9306ACS-277,17,17 Watts,1450,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9350AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SWC-LH9350AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9350AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SWC-LH9350AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9350ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SWC-LH9350ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9350ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SWC-LH9350ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9351AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SWC-LH9351AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9351AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SWC-LH9351AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9351ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SWC-LH9351ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9351ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SWC-LH9351ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9352AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SWC-LH9352AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9352AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SWC-LH9352AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9352ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SWC-LH9352ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9352ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SWC-LH9352ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9354AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SWC-LH9354AS_,17,17 Watts,1450,3500,120,120 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9354AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SWC-LH9354AS-277,17,17 Watts,1450,3500,277,277 Volt,103017649CHI-040 GB E3SFF-LH9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9354ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SWC-LH9354ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9354ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SWC-LH9354ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9356AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SWC-LH9356AS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9356AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SWC-LH9356AS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9356ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SWC-LH9356ACS_,17,17 Watts,1450,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LH9356ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SWC-LH9356ACS-277,17,17 Watts,1450,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,85,17,3,1,0,0
E3SWC-LHWD0AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LHWD0AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD0AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LHWD0AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD0ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LHWD0ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD0ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LHWD0ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD1AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LHWD1AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD1AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LHWD1AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD1ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LHWD1ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD1ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LHWD1ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD2AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LHWD2AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD2AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LHWD2AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD2ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LHWD2ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD2ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LHWD2ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD4AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LHWD4AS_,17,17 Watts,1300,3000,120,120 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD4AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LHWD4AS-277,17,17 Watts,1300,3000,277,277 Volt,102171228CHI-093 GB E3SFF-LHWD4AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD4ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LHWD4ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD4ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LHWD4ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD6AS_,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LHWD6AS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD6AS-277,Wood Ceiling,"High Output , 7W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LHWD6AS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD6ACS_,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LHWD6ACS_,17,17 Watts,1300,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LHWD6ACS-277,Wood Ceiling,"High Output , 7W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LHWD6ACS-277,17,17 Watts,1300,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,76,17,3,1,0,0
E3SWC-LO8270AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SWC-LO8270AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8270AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",10°,E3SWC-LO8270AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8270ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SWC-LO8270ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8270ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",10°,E3SWC-LO8270ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8271AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SWC-LO8271AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8271AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",18°,E3SWC-LO8271AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8271ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SWC-LO8271ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8271ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",18°,E3SWC-LO8271ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8272AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SWC-LO8272AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8272AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",25°,E3SWC-LO8272AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8272ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SWC-LO8272ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8272ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",25°,E3SWC-LO8272ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8274AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SWC-LO8274AS_,12,12 Watts,1319,2700,120,120 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8274AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",40°,E3SWC-LO8274AS-277,12,12 Watts,1319,2700,277,277 Volt,103017649CHI-035 GB E3SFF-LO8274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8274ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SWC-LO8274ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8274ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",40°,E3SWC-LO8274ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8276AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SWC-LO8276AS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8276AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 2700K, 2-Step",60°,E3SWC-LO8276AS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8276ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SWC-LO8276ACS_,12,12 Watts,1319,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8276ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 2700K, 2-Step",60°,E3SWC-LO8276ACS-277,12,12 Watts,1319,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8300AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SWC-LO8300AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8300AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",10°,E3SWC-LO8300AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8300ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SWC-LO8300ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8300ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",10°,E3SWC-LO8300ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8301AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SWC-LO8301AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8301AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",18°,E3SWC-LO8301AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-031 GB E3SFF-LO8301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8301ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SWC-LO8301ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8301ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",18°,E3SWC-LO8301ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8302AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SWC-LO8302AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8302AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",25°,E3SWC-LO8302AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-027 GB E3SFF-LO8302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8302ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SWC-LO8302ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8302ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",25°,E3SWC-LO8302ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8304AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SWC-LO8304AS_,12,12 Watts,1319,3000,120,120 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8304AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",40°,E3SWC-LO8304AS-277,12,12 Watts,1319,3000,277,277 Volt,103017649CHI-023 GB E3SFF-LO8304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8304ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SWC-LO8304ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8304ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",40°,E3SWC-LO8304ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8306AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SWC-LO8306AS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8306AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3000K, 2-Step",60°,E3SWC-LO8306AS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8306ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SWC-LO8306ACS_,12,12 Watts,1319,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8306ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3000K, 2-Step",60°,E3SWC-LO8306ACS-277,12,12 Watts,1319,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8350AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SWC-LO8350AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8350AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",10°,E3SWC-LO8350AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8350ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SWC-LO8350ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8350ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",10°,E3SWC-LO8350ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8351AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SWC-LO8351AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8351AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",18°,E3SWC-LO8351AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8351ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SWC-LO8351ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8351ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",18°,E3SWC-LO8351ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8352AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SWC-LO8352AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8352AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",25°,E3SWC-LO8352AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8352ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SWC-LO8352ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8352ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",25°,E3SWC-LO8352ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8354AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SWC-LO8354AS_,12,12 Watts,1319,3500,120,120 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8354AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",40°,E3SWC-LO8354AS-277,12,12 Watts,1319,3500,277,277 Volt,103017649CHI-039 GB E3SFF-LO8354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8354ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SWC-LO8354ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8354ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",40°,E3SWC-LO8354ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8356AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SWC-LO8356AS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8356AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"80 CRI, 3500K, 2-Step",60°,E3SWC-LO8356AS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8356ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SWC-LO8356ACS_,12,12 Watts,1319,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO8356ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"80 CRI, 3500K, 2-Step",60°,E3SWC-LO8356ACS-277,12,12 Watts,1319,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,110,12,3,0,1,0
E3SWC-LO9270AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SWC-LO9270AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9270AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",10°,E3SWC-LO9270AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9270ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SWC-LO9270ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9270ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",10°,E3SWC-LO9270ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9271AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SWC-LO9271AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9271AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",18°,E3SWC-LO9271AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9271ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SWC-LO9271ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9271ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",18°,E3SWC-LO9271ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9272AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SWC-LO9272AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9272AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",25°,E3SWC-LO9272AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9272ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SWC-LO9272ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9272ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",25°,E3SWC-LO9272ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9274AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SWC-LO9274AS_,12,12 Watts,1124,2700,120,120 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9274AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",40°,E3SWC-LO9274AS-277,12,12 Watts,1124,2700,277,277 Volt,103017649CHI-037 GB E3SFF-LO9274AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9274ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SWC-LO9274ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9274ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",40°,E3SWC-LO9274ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9276AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SWC-LO9276AS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9276AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 2700K, 2-Step",60°,E3SWC-LO9276AS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9276ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SWC-LO9276ACS_,12,12 Watts,1124,2700,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9276ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 2700K, 2-Step",60°,E3SWC-LO9276ACS-277,12,12 Watts,1124,2700,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9300AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SWC-LO9300AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9300AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",10°,E3SWC-LO9300AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9300ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SWC-LO9300ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9300ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",10°,E3SWC-LO9300ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9301AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SWC-LO9301AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9301AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",18°,E3SWC-LO9301AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-033 GB E3SFF-LO9301AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9301ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SWC-LO9301ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9301ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",18°,E3SWC-LO9301ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9302AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SWC-LO9302AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9302AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",25°,E3SWC-LO9302AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-029 GB E3SFF-LO9302AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9302ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SWC-LO9302ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9302ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",25°,E3SWC-LO9302ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9304AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SWC-LO9304AS_,12,12 Watts,1124,3000,120,120 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9304AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",40°,E3SWC-LO9304AS-277,12,12 Watts,1124,3000,277,277 Volt,103017649CHI-025 GB E3SFF-LO9304AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9304ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SWC-LO9304ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9304ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",40°,E3SWC-LO9304ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9306AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SWC-LO9306AS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9306AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000K, 2-Step",60°,E3SWC-LO9306AS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9306ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SWC-LO9306ACS_,12,12 Watts,1124,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9306ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000K, 2-Step",60°,E3SWC-LO9306ACS-277,12,12 Watts,1124,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9350AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SWC-LO9350AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9350AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",10°,E3SWC-LO9350AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9350ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SWC-LO9350ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9350ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",10°,E3SWC-LO9350ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9351AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SWC-LO9351AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9351AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",18°,E3SWC-LO9351AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9351ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SWC-LO9351ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9351ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",18°,E3SWC-LO9351ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9352AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SWC-LO9352AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9352AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",25°,E3SWC-LO9352AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9352ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SWC-LO9352ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9352ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",25°,E3SWC-LO9352ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9354AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SWC-LO9354AS_,12,12 Watts,1124,3500,120,120 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9354AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",40°,E3SWC-LO9354AS-277,12,12 Watts,1124,3500,277,277 Volt,103017649CHI-041 GB E3SFF-LO9354AN.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9354ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SWC-LO9354ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9354ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",40°,E3SWC-LO9354ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9356AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SWC-LO9356AS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9356AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3500K, 2-Step",60°,E3SWC-LO9356AS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9356ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SWC-LO9356ACS_,12,12 Watts,1124,3500,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LO9356ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3500K, 2-Step",60°,E3SWC-LO9356ACS-277,12,12 Watts,1124,3500,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,94,12,3,0,1,0
E3SWC-LOWD0AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LOWD0AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD0AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LOWD0AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD0ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LOWD0ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD0ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",10°,E3SWC-LOWD0ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD1AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LOWD1AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD1AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LOWD1AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD1ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LOWD1ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD1ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",18°,E3SWC-LOWD1ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD2AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LOWD2AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD2AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LOWD2AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD2ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LOWD2ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD2ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",25°,E3SWC-LOWD2ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD4AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LOWD4AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD4AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LOWD4AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD4ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LOWD4ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD4ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",40°,E3SWC-LOWD4ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD6AS_,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LOWD6AS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD6AS-277,Wood Ceiling,"Low Output, 12W",Low Profile IC/Non-IC Airtight,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LOWD6AS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD6ACS_,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LOWD6ACS_,12,12 Watts,900,3000,120,120 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
E3SWC-LOWD6ACS-277,Wood Ceiling,"Low Output, 12W",Low Profile Chicago Plenum,"90 CRI, 3000-1800K, WARM DIM, 3-STEP",60°,E3SWC-LOWD6ACS-277,12,12 Watts,900,3000,277,277 Volt,generic.ies,http://www.element-lighting.com/i//Configurator/2/specsheets/3in_LED_lowprofile_adj_down.pdf,http://www.element-lighting.com/Products/Details/3-LED-Low-Profile-Adjustable-Downlight,http://www.element-lighting.com/i//ELEMENT/documents/Instructions/920E3LED-AS.pdf,75,12,3,0,1,0
