,Mounting##Other##,Output##Other##,"CRI, CCT##Other##",Housing Type##OTHER##,Model##OTHER##,Trim Model##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Voltage Comment##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Photometric Web File##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,C Flanged##OTHER##,C Trim Finish##OTHER##,C Trim Style##OTHER##,C High Output##OTHER##
E3RFW-LHC (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHC (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHC (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHC (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHC (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHC (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHC (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHC (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHC (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHC (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHC (Trim: E3RFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC (Trim: E3RFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC (Trim: E3RFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC (Trim: E3RFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC (Trim: E3RFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHC (Trim: E3RFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHC (Trim: E3RFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHC (Trim: E3RFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHC (Trim: E3RFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHC (Trim: E3RFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHC (Trim: E3RFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHC (Trim: E3RFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC,E3RFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHC-277 (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHC-277 (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHC-277 (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHC-277 (Trim: E3RFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHC-277 (Trim: E3RFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHC-277 (Trim: E3RFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHC-277 (Trim: E3RFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LHC-277,E3RFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHI (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHI (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHI (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHI (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHI (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHI (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHI (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHI (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHI (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHI (Trim: E3RFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI (Trim: E3RFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI (Trim: E3RFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI (Trim: E3RFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI (Trim: E3RFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RFW-LHI (Trim: E3RFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RFW-LHI (Trim: E3RFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RFW-LHI (Trim: E3RFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI,E3RFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RFW-LHI (Trim: E3RFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RFW-LHI (Trim: E3RFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RFW-LHI (Trim: E3RFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RFW-LHI (Trim: E3RFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI,E3RFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHI-277 (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHI-277 (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHI-277 (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RFW-LHI-277 (Trim: E3RFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RFW-LHI-277 (Trim: E3RFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RFW-LHI-277 (Trim: E3RFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RFW-LHI-277 (Trim: E3RFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LHI-277,E3RFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RFW-LOC (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOC (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOC (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOC (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOC (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOC (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOC (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOC (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOC (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOC (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOC (Trim: E3RFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOC (Trim: E3RFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOC (Trim: E3RFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOC (Trim: E3RFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOC (Trim: E3RFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOC (Trim: E3RFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOC (Trim: E3RFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOC (Trim: E3RFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOC (Trim: E3RFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOC (Trim: E3RFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOC (Trim: E3RFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOC (Trim: E3RFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC,E3RFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOC-277 (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOC-277 (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOC-277 (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOC-277 (Trim: E3RFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOC-277 (Trim: E3RFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOC-277 (Trim: E3RFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOC-277 (Trim: E3RFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RFW-LOC-277,E3RFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOI (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOI (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOI (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOI (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOI (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOI (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOI (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOI (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOI (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOI (Trim: E3RFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RFW-LOI (Trim: E3RFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RFW-LOI (Trim: E3RFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RFW-LOI (Trim: E3RFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RFW-LOI (Trim: E3RFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RFW-LOI (Trim: E3RFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RFW-LOI (Trim: E3RFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RFW-LOI (Trim: E3RFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI,E3RFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RFW-LOI (Trim: E3RFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RFW-LOI (Trim: E3RFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RFW-LOI (Trim: E3RFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RFW-LOI (Trim: E3RFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI,E3RFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOI-277 (Trim: E3RF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOI-277 (Trim: E3RF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOI-277 (Trim: E3RF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RFW-LOI-277 (Trim: E3RFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RFW-LOI-277 (Trim: E3RFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RFW-LOI-277 (Trim: E3RFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RFW-LOI-277 (Trim: E3RFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RFW-LOI-277,E3RFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RLW-LHC (Trim: E3RLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,2,1,1
E3RLW-LHC (Trim: E3RLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,3,1,1
E3RLW-LHC (Trim: E3RLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,4,1,1
E3RLW-LHC (Trim: E3RLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,1,1,1
E3RLW-LHC (Trim: E3RLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-830-B,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,2,1,1
E3RLW-LHC (Trim: E3RLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-830-S,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,3,1,1
E3RLW-LHC (Trim: E3RLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-830-W,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,4,1,1
E3RLW-LHC (Trim: E3RLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,1,1,1
E3RLW-LHC (Trim: E3RLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,2,1,1
E3RLW-LHC (Trim: E3RLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,3,1,1
E3RLW-LHC (Trim: E3RLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,4,1,1
E3RLW-LHC (Trim: E3RLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,1,1,1
E3RLW-LHC (Trim: E3RLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHC (Trim: E3RLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHC (Trim: E3RLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHC (Trim: E3RLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHC (Trim: E3RLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHC (Trim: E3RLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHC (Trim: E3RLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHC (Trim: E3RLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHC (Trim: E3RLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHC (Trim: E3RLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHC (Trim: E3RLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHC (Trim: E3RLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHC (Trim: E3RLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,2,1,1
E3RLW-LHC (Trim: E3RLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,3,1,1
E3RLW-LHC (Trim: E3RLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,4,1,1
E3RLW-LHC (Trim: E3RLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC,E3RLW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-830-B,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-830-S,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-830-W,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHC-277 (Trim: E3RLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,2,1,1
E3RLW-LHC-277 (Trim: E3RLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,3,1,1
E3RLW-LHC-277 (Trim: E3RLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,4,1,1
E3RLW-LHC-277 (Trim: E3RLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LHC-277,E3RLW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,1,1,1
E3RLW-LHI (Trim: E3RLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,2,1,1
E3RLW-LHI (Trim: E3RLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,3,1,1
E3RLW-LHI (Trim: E3RLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,4,1,1
E3RLW-LHI (Trim: E3RLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,1,1,1
E3RLW-LHI (Trim: E3RLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-830-B,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,2,1,1
E3RLW-LHI (Trim: E3RLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-830-S,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,3,1,1
E3RLW-LHI (Trim: E3RLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-830-W,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,4,1,1
E3RLW-LHI (Trim: E3RLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,1,1,1
E3RLW-LHI (Trim: E3RLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,2,1,1
E3RLW-LHI (Trim: E3RLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,3,1,1
E3RLW-LHI (Trim: E3RLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,4,1,1
E3RLW-LHI (Trim: E3RLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,1,1,1
E3RLW-LHI (Trim: E3RLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHI (Trim: E3RLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHI (Trim: E3RLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHI (Trim: E3RLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHI (Trim: E3RLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHI (Trim: E3RLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHI (Trim: E3RLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHI (Trim: E3RLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHI (Trim: E3RLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,2,1,1
E3RLW-LHI (Trim: E3RLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,3,1,1
E3RLW-LHI (Trim: E3RLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,4,1,1
E3RLW-LHI (Trim: E3RLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI,E3RLW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,1,1,1
E3RLW-LHI (Trim: E3RLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI,E3RLW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,2,1,1
E3RLW-LHI (Trim: E3RLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI,E3RLW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,3,1,1
E3RLW-LHI (Trim: E3RLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI,E3RLW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,4,1,1
E3RLW-LHI (Trim: E3RLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI,E3RLW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-830-B,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-830-S,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-830-W,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,1,1,1
E3RLW-LHI-277 (Trim: E3RLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,2,1,1
E3RLW-LHI-277 (Trim: E3RLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,3,1,1
E3RLW-LHI-277 (Trim: E3RLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,4,1,1
E3RLW-LHI-277 (Trim: E3RLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LHI-277,E3RLW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,1,1,1
E3RLW-LOC (Trim: E3RLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,2,1,0
E3RLW-LOC (Trim: E3RLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,3,1,0
E3RLW-LOC (Trim: E3RLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,4,1,0
E3RLW-LOC (Trim: E3RLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,1,1,0
E3RLW-LOC (Trim: E3RLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-830-B,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,2,1,0
E3RLW-LOC (Trim: E3RLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-830-S,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,3,1,0
E3RLW-LOC (Trim: E3RLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-830-W,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,4,1,0
E3RLW-LOC (Trim: E3RLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-830-Z,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,1,1,0
E3RLW-LOC (Trim: E3RLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,2,1,0
E3RLW-LOC (Trim: E3RLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,3,1,0
E3RLW-LOC (Trim: E3RLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,4,1,0
E3RLW-LOC (Trim: E3RLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,1,1,0
E3RLW-LOC (Trim: E3RLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOC (Trim: E3RLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOC (Trim: E3RLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOC (Trim: E3RLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOC (Trim: E3RLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOC (Trim: E3RLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOC (Trim: E3RLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOC (Trim: E3RLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOC (Trim: E3RLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOC (Trim: E3RLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOC (Trim: E3RLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOC (Trim: E3RLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOC (Trim: E3RLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,2,1,0
E3RLW-LOC (Trim: E3RLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,3,1,0
E3RLW-LOC (Trim: E3RLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,4,1,0
E3RLW-LOC (Trim: E3RLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC,E3RLW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-830-B,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-830-S,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-830-W,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-830-Z,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOC-277 (Trim: E3RLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,2,1,0
E3RLW-LOC-277 (Trim: E3RLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,3,1,0
E3RLW-LOC-277 (Trim: E3RLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,4,1,0
E3RLW-LOC-277 (Trim: E3RLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RLW-LOC-277,E3RLW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,1,1,0
E3RLW-LOI (Trim: E3RLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,2,1,0
E3RLW-LOI (Trim: E3RLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,3,1,0
E3RLW-LOI (Trim: E3RLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,4,1,0
E3RLW-LOI (Trim: E3RLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,1,1,0
E3RLW-LOI (Trim: E3RLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-830-B,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,2,1,0
E3RLW-LOI (Trim: E3RLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-830-S,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,3,1,0
E3RLW-LOI (Trim: E3RLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-830-W,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,4,1,0
E3RLW-LOI (Trim: E3RLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-830-Z,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,1,1,0
E3RLW-LOI (Trim: E3RLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,2,1,0
E3RLW-LOI (Trim: E3RLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,3,1,0
E3RLW-LOI (Trim: E3RLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,4,1,0
E3RLW-LOI (Trim: E3RLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,1,1,0
E3RLW-LOI (Trim: E3RLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOI (Trim: E3RLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOI (Trim: E3RLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOI (Trim: E3RLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOI (Trim: E3RLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOI (Trim: E3RLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOI (Trim: E3RLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOI (Trim: E3RLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOI (Trim: E3RLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,2,1,0
E3RLW-LOI (Trim: E3RLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,3,1,0
E3RLW-LOI (Trim: E3RLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,4,1,0
E3RLW-LOI (Trim: E3RLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI,E3RLW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,1,1,0
E3RLW-LOI (Trim: E3RLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI,E3RLW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,2,1,0
E3RLW-LOI (Trim: E3RLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI,E3RLW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,3,1,0
E3RLW-LOI (Trim: E3RLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI,E3RLW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,4,1,0
E3RLW-LOI (Trim: E3RLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI,E3RLW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-830-B,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-830-S,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-830-W,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-830-Z,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,1,1,0
E3RLW-LOI-277 (Trim: E3RLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,2,1,0
E3RLW-LOI-277 (Trim: E3RLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,3,1,0
E3RLW-LOI-277 (Trim: E3RLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,4,1,0
E3RLW-LOI-277 (Trim: E3RLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RLW-LOI-277,E3RLW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,1,1,0
E3RWCW-LHC (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHC (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHC (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHC (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHC (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHC (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHC (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHC (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHC (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHC (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHC (Trim: E3RFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHC (Trim: E3RFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHC (Trim: E3RFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHC (Trim: E3RFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC,E3RFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHC-277 (Trim: E3RFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHC-277 (Trim: E3RFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHC-277 (Trim: E3RFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHC-277 (Trim: E3RFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LHC-277,E3RFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHI (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHI (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHI (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHI (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHI (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHI (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHI (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHI (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHI (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI,E3RFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,2,1
E3RWCW-LHI (Trim: E3RFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,2,1
E3RWCW-LHI (Trim: E3RFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,2,1
E3RWCW-LHI (Trim: E3RFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,2,1
E3RWCW-LHI (Trim: E3RFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI,E3RFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,2,1
E3RWCW-LHI-277 (Trim: E3RFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,2,1
E3RWCW-LHI-277 (Trim: E3RFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,2,1
E3RWCW-LHI-277 (Trim: E3RFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,2,1
E3RWCW-LHI-277 (Trim: E3RFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LHI-277,E3RFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,2,1
E3RWCW-LOC (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOC (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOC (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOC (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOC (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOC (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOC (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOC (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOC (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOC (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOC (Trim: E3RFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOC (Trim: E3RFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOC (Trim: E3RFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOC (Trim: E3RFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC,E3RFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOC-277 (Trim: E3RFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOC-277 (Trim: E3RFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOC-277 (Trim: E3RFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOC-277 (Trim: E3RFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3RWCW-LOC-277,E3RFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOI (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOI (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOI (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOI (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOI (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOI (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOI (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOI (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOI (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI,E3RFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,2,0
E3RWCW-LOI (Trim: E3RFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,2,0
E3RWCW-LOI (Trim: E3RFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,2,0
E3RWCW-LOI (Trim: E3RFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,2,0
E3RWCW-LOI (Trim: E3RFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI,E3RFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,2,0
E3RWCW-LOI-277 (Trim: E3RFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,2,0
E3RWCW-LOI-277 (Trim: E3RFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,2,0
E3RWCW-LOI-277 (Trim: E3RFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,2,0
E3RWCW-LOI-277 (Trim: E3RFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3RWCW-LOI-277,E3RFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,2,0
E3SFW-LHC (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHC (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHC (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHC (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHC (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHC (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHC (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHC (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHC (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHC (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHC (Trim: E3SFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC (Trim: E3SFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC (Trim: E3SFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC (Trim: E3SFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC (Trim: E3SFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHC (Trim: E3SFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHC (Trim: E3SFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHC (Trim: E3SFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHC (Trim: E3SFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHC (Trim: E3SFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHC (Trim: E3SFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHC (Trim: E3SFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC,E3SFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHC-277 (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHC-277 (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHC-277 (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHC-277 (Trim: E3SFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHC-277 (Trim: E3SFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHC-277 (Trim: E3SFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHC-277 (Trim: E3SFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LHC-277,E3SFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHI (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHI (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHI (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHI (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHI (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHI (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHI (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHI (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHI (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHI (Trim: E3SFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-827-B,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-827-S,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-827-W,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-830-B,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-830-S,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-830-W,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-835-B,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI (Trim: E3SFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-835-S,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI (Trim: E3SFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-835-W,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI (Trim: E3SFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI (Trim: E3SFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-930-B,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-930-S,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-930-W,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-930-Z,17,17 Watts,942,3000,120 Volt,120,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SFW-LHI (Trim: E3SFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SFW-LHI (Trim: E3SFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SFW-LHI (Trim: E3SFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI,E3SFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SFW-LHI (Trim: E3SFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SFW-LHI (Trim: E3SFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SFW-LHI (Trim: E3SFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SFW-LHI (Trim: E3SFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI,E3SFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHI-277 (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHI-277 (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHI-277 (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-827-B),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-827-B,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-827-S),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-827-S,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-827-W),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-827-W,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-827-Z),Flanged,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,103017649CHI-013 GB E3SFW-LH827N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-830-B),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-830-B,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-830-S),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-830-S,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-830-W),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-830-W,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-830-Z),Flanged,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103017649CHI-009 GB E3SFW-LH830N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-835-B),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-835-B,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-835-S),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-835-S,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-835-W),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-835-W,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-835-Z),Flanged,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,103017649CHI-014 GB E3SFW-LH835N.ies,79,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-927-B),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-927-S),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-927-W),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-927-Z),Flanged,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-930-B),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-930-B,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-930-S),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-930-S,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-930-W),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-930-W,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-930-Z),Flanged,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-930-Z,17,17 Watts,942,3000,277 Volt,277,103017649CHI-011 GB E3SFW-LH930N.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-935-B),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-935-S),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-935-W),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-935-Z),Flanged,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SFW-LHI-277 (Trim: E3SFW-WD-B),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SFW-LHI-277 (Trim: E3SFW-WD-S),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SFW-LHI-277 (Trim: E3SFW-WD-W),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SFW-LHI-277 (Trim: E3SFW-WD-Z),Flanged,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LHI-277,E3SFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SFW-LOC (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOC (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOC (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOC (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOC (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOC (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOC (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOC (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOC (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOC (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOC (Trim: E3SFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOC (Trim: E3SFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOC (Trim: E3SFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOC (Trim: E3SFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOC (Trim: E3SFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOC (Trim: E3SFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOC (Trim: E3SFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOC (Trim: E3SFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOC (Trim: E3SFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOC (Trim: E3SFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOC (Trim: E3SFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOC (Trim: E3SFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC,E3SFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOC-277 (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOC-277 (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOC-277 (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOC-277 (Trim: E3SFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOC-277 (Trim: E3SFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOC-277 (Trim: E3SFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOC-277 (Trim: E3SFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SFW-LOC-277,E3SFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOI (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOI (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOI (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOI (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOI (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOI (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOI (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOI (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOI (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOI (Trim: E3SFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-830-B,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-830-S,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-830-W,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-830-Z,12,12 Watts,853,3000,120 Volt,120,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SFW-LOI (Trim: E3SFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SFW-LOI (Trim: E3SFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SFW-LOI (Trim: E3SFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SFW-LOI (Trim: E3SFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-930-B,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-930-S,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-930-W,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-930-Z,12,12 Watts,675,3000,120 Volt,120,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SFW-LOI (Trim: E3SFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SFW-LOI (Trim: E3SFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SFW-LOI (Trim: E3SFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI,E3SFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SFW-LOI (Trim: E3SFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SFW-LOI (Trim: E3SFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SFW-LOI (Trim: E3SFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SFW-LOI (Trim: E3SFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI,E3SFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-827-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-827-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-827-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-827-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-830-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-830-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-830-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-830-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-835-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-835-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-835-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-835-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-927-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-927-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-927-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-927-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-930-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-930-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-930-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-930-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-935-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-935-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-935-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-935-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF15W-WD-B),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF15W-WD-S),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF15W-WD-W),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF15W-WD-Z),"Flanged 1.1""-1.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-827-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-827-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-827-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-827-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-830-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-830-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-830-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-830-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-835-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-835-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-835-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-835-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-927-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-927-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-927-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-927-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-930-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-930-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-930-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-930-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-935-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-935-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-935-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-935-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF20W-WD-B),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF20W-WD-S),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF20W-WD-W),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF20W-WD-Z),"Flanged 1.6""-2.0"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-827-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-827-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-827-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-827-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-830-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-830-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-830-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-830-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-835-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-835-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-835-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-835-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-927-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-927-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-927-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-927-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-930-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-930-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-930-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-930-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-935-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-935-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-935-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-935-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SF25W-WD-B),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOI-277 (Trim: E3SF25W-WD-S),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOI-277 (Trim: E3SF25W-WD-W),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOI-277 (Trim: E3SF25W-WD-Z),"Flanged 2.1""-2.5"" Ceiling Thickness",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-827-B),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-827-S),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-827-W),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-827-Z),Flanged,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-830-B),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-830-B,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-830-S),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-830-S,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-830-W),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-830-W,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-830-Z),Flanged,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-830-Z,12,12 Watts,853,3000,277 Volt,277,103017649CHI-010 GB E3SFW-LO830N.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-835-B),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-835-S),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-835-W),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-835-Z),Flanged,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-927-B),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-927-S),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-927-W),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-927-Z),Flanged,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-930-B),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-930-B,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-930-S),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-930-S,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-930-W),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-930-W,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-930-Z),Flanged,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-930-Z,12,12 Watts,675,3000,277 Volt,277,103017649CHI-012 GB E3SFW-LO930N.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-935-B),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-935-S),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-935-W),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-935-Z),Flanged,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SFW-LOI-277 (Trim: E3SFW-WD-B),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SFW-LOI-277 (Trim: E3SFW-WD-S),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SFW-LOI-277 (Trim: E3SFW-WD-W),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SFW-LOI-277 (Trim: E3SFW-WD-Z),Flanged,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SFW-LOI-277,E3SFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SLW-LHC (Trim: E3SLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,2,3,1
E3SLW-LHC (Trim: E3SLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,3,3,1
E3SLW-LHC (Trim: E3SLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,4,3,1
E3SLW-LHC (Trim: E3SLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,1,3,1
E3SLW-LHC (Trim: E3SLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-830-B,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,2,3,1
E3SLW-LHC (Trim: E3SLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-830-S,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,3,3,1
E3SLW-LHC (Trim: E3SLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-830-W,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,4,3,1
E3SLW-LHC (Trim: E3SLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,1,3,1
E3SLW-LHC (Trim: E3SLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,2,3,1
E3SLW-LHC (Trim: E3SLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,3,3,1
E3SLW-LHC (Trim: E3SLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,4,3,1
E3SLW-LHC (Trim: E3SLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,1,3,1
E3SLW-LHC (Trim: E3SLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHC (Trim: E3SLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHC (Trim: E3SLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHC (Trim: E3SLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHC (Trim: E3SLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHC (Trim: E3SLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHC (Trim: E3SLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHC (Trim: E3SLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHC (Trim: E3SLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHC (Trim: E3SLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHC (Trim: E3SLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHC (Trim: E3SLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHC (Trim: E3SLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,2,3,1
E3SLW-LHC (Trim: E3SLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,3,3,1
E3SLW-LHC (Trim: E3SLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,4,3,1
E3SLW-LHC (Trim: E3SLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC,E3SLW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-830-B,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-830-S,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-830-W,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHC-277 (Trim: E3SLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,2,3,1
E3SLW-LHC-277 (Trim: E3SLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,3,3,1
E3SLW-LHC-277 (Trim: E3SLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,4,3,1
E3SLW-LHC-277 (Trim: E3SLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LHC-277,E3SLW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,1,3,1
E3SLW-LHI (Trim: E3SLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,2,3,1
E3SLW-LHI (Trim: E3SLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,3,3,1
E3SLW-LHI (Trim: E3SLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,4,3,1
E3SLW-LHI (Trim: E3SLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,0,1,3,1
E3SLW-LHI (Trim: E3SLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-830-B,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,2,3,1
E3SLW-LHI (Trim: E3SLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-830-S,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,3,3,1
E3SLW-LHI (Trim: E3SLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-830-W,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,4,3,1
E3SLW-LHI (Trim: E3SLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-830-Z,17,17 Watts,1342,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,79,0,1,3,1
E3SLW-LHI (Trim: E3SLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,2,3,1
E3SLW-LHI (Trim: E3SLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,3,3,1
E3SLW-LHI (Trim: E3SLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,4,3,1
E3SLW-LHI (Trim: E3SLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,0,1,3,1
E3SLW-LHI (Trim: E3SLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHI (Trim: E3SLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHI (Trim: E3SLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHI (Trim: E3SLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHI (Trim: E3SLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHI (Trim: E3SLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHI (Trim: E3SLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHI (Trim: E3SLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHI (Trim: E3SLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,2,3,1
E3SLW-LHI (Trim: E3SLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,3,3,1
E3SLW-LHI (Trim: E3SLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,4,3,1
E3SLW-LHI (Trim: E3SLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI,E3SLW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,0,1,3,1
E3SLW-LHI (Trim: E3SLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI,E3SLW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,2,3,1
E3SLW-LHI (Trim: E3SLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI,E3SLW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,3,3,1
E3SLW-LHI (Trim: E3SLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI,E3SLW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,4,3,1
E3SLW-LHI (Trim: E3SLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI,E3SLW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-827-B),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-827-S),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-827-W),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-827-Z),Flangeless,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-830-B),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-830-B,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-830-S),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-830-S,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-830-W),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-830-W,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-830-Z),Flangeless,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-830-Z,17,17 Watts,1342,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,79,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-835-B),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-835-S),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-835-W),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-835-Z),Flangeless,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-927-B),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-927-S),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-927-W),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-927-Z),Flangeless,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-930-B),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-930-S),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-930-W),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-930-Z),Flangeless,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-935-B),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-935-S),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-935-W),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-935-Z),Flangeless,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,0,1,3,1
E3SLW-LHI-277 (Trim: E3SLW-WD-B),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,2,3,1
E3SLW-LHI-277 (Trim: E3SLW-WD-S),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,3,3,1
E3SLW-LHI-277 (Trim: E3SLW-WD-W),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,4,3,1
E3SLW-LHI-277 (Trim: E3SLW-WD-Z),Flangeless,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LHI-277,E3SLW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,0,1,3,1
E3SLW-LOC (Trim: E3SLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,2,3,0
E3SLW-LOC (Trim: E3SLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,3,3,0
E3SLW-LOC (Trim: E3SLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,4,3,0
E3SLW-LOC (Trim: E3SLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,1,3,0
E3SLW-LOC (Trim: E3SLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-830-B,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,2,3,0
E3SLW-LOC (Trim: E3SLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-830-S,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,3,3,0
E3SLW-LOC (Trim: E3SLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-830-W,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,4,3,0
E3SLW-LOC (Trim: E3SLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-830-Z,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,1,3,0
E3SLW-LOC (Trim: E3SLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,2,3,0
E3SLW-LOC (Trim: E3SLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,3,3,0
E3SLW-LOC (Trim: E3SLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,4,3,0
E3SLW-LOC (Trim: E3SLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,1,3,0
E3SLW-LOC (Trim: E3SLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOC (Trim: E3SLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOC (Trim: E3SLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOC (Trim: E3SLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOC (Trim: E3SLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOC (Trim: E3SLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOC (Trim: E3SLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOC (Trim: E3SLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOC (Trim: E3SLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOC (Trim: E3SLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOC (Trim: E3SLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOC (Trim: E3SLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOC (Trim: E3SLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,2,3,0
E3SLW-LOC (Trim: E3SLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,3,3,0
E3SLW-LOC (Trim: E3SLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,4,3,0
E3SLW-LOC (Trim: E3SLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC,E3SLW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-830-B,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-830-S,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-830-W,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-830-Z,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOC-277 (Trim: E3SLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,2,3,0
E3SLW-LOC-277 (Trim: E3SLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,3,3,0
E3SLW-LOC-277 (Trim: E3SLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,4,3,0
E3SLW-LOC-277 (Trim: E3SLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SLW-LOC-277,E3SLW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,1,3,0
E3SLW-LOI (Trim: E3SLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,2,3,0
E3SLW-LOI (Trim: E3SLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,3,3,0
E3SLW-LOI (Trim: E3SLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,4,3,0
E3SLW-LOI (Trim: E3SLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,0,1,3,0
E3SLW-LOI (Trim: E3SLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-830-B,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,2,3,0
E3SLW-LOI (Trim: E3SLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-830-S,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,3,3,0
E3SLW-LOI (Trim: E3SLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-830-W,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,4,3,0
E3SLW-LOI (Trim: E3SLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-830-Z,12,12 Watts,853,3000,120 Volt,120,103643585CHI-010A E3SLW-830-W.ies,70,0,1,3,0
E3SLW-LOI (Trim: E3SLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,2,3,0
E3SLW-LOI (Trim: E3SLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,3,3,0
E3SLW-LOI (Trim: E3SLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,4,3,0
E3SLW-LOI (Trim: E3SLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,0,1,3,0
E3SLW-LOI (Trim: E3SLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOI (Trim: E3SLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOI (Trim: E3SLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOI (Trim: E3SLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOI (Trim: E3SLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOI (Trim: E3SLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOI (Trim: E3SLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOI (Trim: E3SLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOI (Trim: E3SLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,2,3,0
E3SLW-LOI (Trim: E3SLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,3,3,0
E3SLW-LOI (Trim: E3SLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,4,3,0
E3SLW-LOI (Trim: E3SLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI,E3SLW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,0,1,3,0
E3SLW-LOI (Trim: E3SLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI,E3SLW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,2,3,0
E3SLW-LOI (Trim: E3SLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI,E3SLW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,3,3,0
E3SLW-LOI (Trim: E3SLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI,E3SLW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,4,3,0
E3SLW-LOI (Trim: E3SLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI,E3SLW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-827-B),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-827-S),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-827-W),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-827-Z),Flangeless,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-830-B),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-830-B,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-830-S),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-830-S,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-830-W),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-830-W,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-830-Z),Flangeless,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-830-Z,12,12 Watts,853,3000,277 Volt,277,103643585CHI-010A E3SLW-830-W.ies,70,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-835-B),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-835-S),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-835-W),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-835-Z),Flangeless,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-927-B),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-927-S),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-927-W),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-927-Z),Flangeless,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-930-B),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-930-S),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-930-W),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-930-Z),Flangeless,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-935-B),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-935-S),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-935-W),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-935-Z),Flangeless,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,0,1,3,0
E3SLW-LOI-277 (Trim: E3SLW-WD-B),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,2,3,0
E3SLW-LOI-277 (Trim: E3SLW-WD-S),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,3,3,0
E3SLW-LOI-277 (Trim: E3SLW-WD-W),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,4,3,0
E3SLW-LOI-277 (Trim: E3SLW-WD-Z),Flangeless,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SLW-LOI-277,E3SLW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,0,1,3,0
E3SWCW-LHC (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHC (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHC (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHC (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHC (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHC (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHC (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHC (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHC (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHC (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHC (Trim: E3SFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHC (Trim: E3SFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHC (Trim: E3SFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHC (Trim: E3SFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC,E3SFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHC-277 (Trim: E3SFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHC-277 (Trim: E3SFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHC-277 (Trim: E3SFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHC-277 (Trim: E3SFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LHC-277,E3SFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHI (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHI (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHI (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF15W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHI (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHI (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHI (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF20W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHI (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHI (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHI (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SF25W-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-827-B,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-827-S,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-827-W,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-827-Z,17,17 Watts,1342,2700,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-830-B,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-830-S,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-830-W,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-830-Z,17,17 Watts,1342,3000,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-835-B,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-835-S,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-835-W,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-835-Z,17,17 Watts,1342,3500,120 Volt,120,generic.ies,79,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-927-B,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-927-S,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-927-W,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-927-Z,17,17 Watts,942,2700,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-930-B,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-930-S,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-930-W,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-930-Z,17,17 Watts,942,3000,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-935-B,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-935-S,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-935-W,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI,E3SFW-935-Z,17,17 Watts,942,3500,120 Volt,120,generic.ies,51,1,1,4,1
E3SWCW-LHI (Trim: E3SFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SFW-WD-B,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,2,4,1
E3SWCW-LHI (Trim: E3SFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SFW-WD-S,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,3,4,1
E3SWCW-LHI (Trim: E3SFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SFW-WD-W,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,4,4,1
E3SWCW-LHI (Trim: E3SFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI,E3SFW-WD-Z,17,17 Watts,900,3000,120 Volt,120,generic.ies,53,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF15W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF20W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SF25W-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-827-B),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-827-B,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-827-S),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-827-S,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-827-W),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-827-W,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-827-Z),Wood Ceiling,High Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-827-Z,17,17 Watts,1342,2700,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-830-B),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-830-B,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-830-S),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-830-S,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-830-W),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-830-W,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-830-Z),Wood Ceiling,High Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-830-Z,17,17 Watts,1342,3000,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-835-B),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-835-B,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-835-S),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-835-S,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-835-W),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-835-W,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-835-Z),Wood Ceiling,High Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-835-Z,17,17 Watts,1342,3500,277 Volt,277,generic.ies,79,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-927-B),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-927-B,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-927-S),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-927-S,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-927-W),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-927-W,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-927-Z),Wood Ceiling,High Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-927-Z,17,17 Watts,942,2700,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-930-B),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-930-B,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-930-S),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-930-S,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-930-W),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-930-W,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-930-Z),Wood Ceiling,High Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-930-Z,17,17 Watts,942,3000,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-935-B),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-935-B,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-935-S),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-935-S,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-935-W),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-935-W,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-935-Z),Wood Ceiling,High Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-935-Z,17,17 Watts,942,3500,277 Volt,277,generic.ies,51,1,1,4,1
E3SWCW-LHI-277 (Trim: E3SFW-WD-B),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-WD-B,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,2,4,1
E3SWCW-LHI-277 (Trim: E3SFW-WD-S),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-WD-S,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,3,4,1
E3SWCW-LHI-277 (Trim: E3SFW-WD-W),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-WD-W,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,4,4,1
E3SWCW-LHI-277 (Trim: E3SFW-WD-Z),Wood Ceiling,High Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LHI-277,E3SFW-WD-Z,17,17 Watts,900,3000,277 Volt,277,generic.ies,53,1,1,4,1
E3SWCW-LOC (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOC (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOC (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOC (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOC (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOC (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOC (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOC (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOC (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOC (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOC (Trim: E3SFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOC (Trim: E3SFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOC (Trim: E3SFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOC (Trim: E3SFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC,E3SFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOC-277 (Trim: E3SFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOC-277 (Trim: E3SFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOC-277 (Trim: E3SFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOC-277 (Trim: E3SFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E3SWCW-LOC-277,E3SFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOI (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOI (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOI (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF15W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOI (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOI (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOI (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF20W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOI (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOI (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOI (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SF25W-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-827-B,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-827-S,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-827-W,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-827-Z,12,12 Watts,853,2700,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-830-B,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-830-S,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-830-W,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-830-Z,12,12 Watts,853,3000,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-835-B,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-835-S,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-835-W,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-835-Z,12,12 Watts,853,3500,120 Volt,120,generic.ies,70,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-927-B,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-927-S,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-927-W,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-927-Z,12,12 Watts,675,2700,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-930-B,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-930-S,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-930-W,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-930-Z,12,12 Watts,675,3000,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-935-B,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-935-S,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-935-W,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI,E3SFW-935-Z,12,12 Watts,675,3500,120 Volt,120,generic.ies,56,1,1,4,0
E3SWCW-LOI (Trim: E3SFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SFW-WD-B,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,2,4,0
E3SWCW-LOI (Trim: E3SFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SFW-WD-S,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,3,4,0
E3SWCW-LOI (Trim: E3SFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SFW-WD-W,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,4,4,0
E3SWCW-LOI (Trim: E3SFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI,E3SFW-WD-Z,12,12 Watts,600,3000,120 Volt,120,generic.ies,50,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-827-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-827-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-827-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-827-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-830-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-830-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-830-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-830-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-835-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-835-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-835-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-835-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-927-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-927-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-927-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-927-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-930-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-930-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-930-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-930-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-935-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-935-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-935-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-935-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-WD-B),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-WD-S),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-WD-W),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF15W-WD-Z),"Wood Ceiling (Flanged 1.1""-1.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF15W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-827-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-827-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-827-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-827-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-830-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-830-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-830-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-830-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-835-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-835-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-835-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-835-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-927-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-927-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-927-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-927-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-930-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-930-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-930-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-930-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-935-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-935-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-935-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-935-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-WD-B),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-WD-S),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-WD-W),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF20W-WD-Z),"Wood Ceiling (Flanged 1.6""-2.0"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF20W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-827-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-827-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-827-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-827-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-830-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-830-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-830-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-830-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-835-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-835-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-835-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-835-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-927-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-927-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-927-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-927-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-930-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-930-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-930-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-930-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-935-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-935-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-935-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-935-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-WD-B),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-WD-S),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-WD-W),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SF25W-WD-Z),"Wood Ceiling (Flanged 2.1""-2.5"" Ceiling Thickness)",Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SF25W-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-827-B),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-827-B,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-827-S),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-827-S,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-827-W),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-827-W,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-827-Z),Wood Ceiling,Low Output 12W,80 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-827-Z,12,12 Watts,853,2700,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-830-B),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-830-B,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-830-S),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-830-S,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-830-W),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-830-W,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-830-Z),Wood Ceiling,Low Output 12W,80 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-830-Z,12,12 Watts,853,3000,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-835-B),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-835-B,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-835-S),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-835-S,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-835-W),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-835-W,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-835-Z),Wood Ceiling,Low Output 12W,80 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-835-Z,12,12 Watts,853,3500,277 Volt,277,generic.ies,70,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-927-B),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-927-B,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-927-S),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-927-S,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-927-W),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-927-W,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-927-Z),Wood Ceiling,Low Output 12W,90 CRI 2700K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-927-Z,12,12 Watts,675,2700,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-930-B),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-930-B,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-930-S),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-930-S,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-930-W),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-930-W,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-930-Z),Wood Ceiling,Low Output 12W,90 CRI 3000K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-930-Z,12,12 Watts,675,3000,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-935-B),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-935-B,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-935-S),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-935-S,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-935-W),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-935-W,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-935-Z),Wood Ceiling,Low Output 12W,90 CRI 3500K 2-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-935-Z,12,12 Watts,675,3500,277 Volt,277,generic.ies,56,1,1,4,0
E3SWCW-LOI-277 (Trim: E3SFW-WD-B),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-WD-B,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,2,4,0
E3SWCW-LOI-277 (Trim: E3SFW-WD-S),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-WD-S,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,3,4,0
E3SWCW-LOI-277 (Trim: E3SFW-WD-W),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-WD-W,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,4,4,0
E3SWCW-LOI-277 (Trim: E3SFW-WD-Z),Wood Ceiling,Low Output 12W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E3SWCW-LOI-277,E3SFW-WD-Z,12,12 Watts,600,3000,277 Volt,277,generic.ies,50,1,1,4,0
