,Mounting##Other##,Output##Other##,"CRI, CCT##Other##",Housing Type##OTHER##,Model##OTHER##,Trim Model##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Wattage Comments##Other##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Voltage Comment##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Photometric Web File##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,C Flanged##OTHER##,C Trim Finish##OTHER##,C Trim Style##OTHER##,C High Output##OTHER##
E4RFW-LHC (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHC (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHC (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHC (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHC (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHC (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHC (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHC (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHC (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHC (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHC (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHC (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHC (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHC (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHC (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHC (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHC (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHC (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHC (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHC (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHC (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHC (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHC (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHC (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHC (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,2,1
E4RFW-LHC (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,2,1
E4RFW-LHC (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,2,1
E4RFW-LHC (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC,E4RFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHC-277 (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,2,1
E4RFW-LHC-277 (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,2,1
E4RFW-LHC-277 (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,2,1
E4RFW-LHC-277 (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LHC-277,E4RFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,2,1
E4RFW-LHI (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHI (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHI (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHI (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHI (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHI (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHI (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHI (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHI (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHI (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHI (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHI (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHI (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHI (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHI (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHI (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHI (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHI (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHI (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHI (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHI (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHI (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHI (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHI (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI,E4RFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHI (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI,E4RFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,2,1
E4RFW-LHI (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI,E4RFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,2,1
E4RFW-LHI (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI,E4RFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,2,1
E4RFW-LHI (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI,E4RFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHI-277 (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,2,1
E4RFW-LHI-277 (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,2,1
E4RFW-LHI-277 (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,2,1
E4RFW-LHI-277 (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LHI-277,E4RFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,2,1
E4RFW-LHN (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHN (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHN (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHN (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHN (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-830-B,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,2,2,1
E4RFW-LHN (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-830-S,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,3,2,1
E4RFW-LHN (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-830-W,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,4,2,1
E4RFW-LHN (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,1,2,1
E4RFW-LHN (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,2,1
E4RFW-LHN (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,2,1
E4RFW-LHN (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,2,1
E4RFW-LHN (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,2,1
E4RFW-LHN (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHN (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHN (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHN (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHN (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-930-B,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,2,2,1
E4RFW-LHN (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-930-S,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,3,2,1
E4RFW-LHN (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-930-W,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,4,2,1
E4RFW-LHN (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,1,2,1
E4RFW-LHN (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,2,1
E4RFW-LHN (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,2,1
E4RFW-LHN (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,2,1
E4RFW-LHN (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,2,1
E4RFW-LHN (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,2,1
E4RFW-LHN (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,2,1
E4RFW-LHN (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,2,1
E4RFW-LHN (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN,E4RFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-830-B,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-830-S,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-830-W,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-930-B,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-930-S,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-930-W,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,2,1
E4RFW-LHN-277 (Trim: E4RFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,2,1
E4RFW-LHN-277 (Trim: E4RFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,2,1
E4RFW-LHN-277 (Trim: E4RFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,2,1
E4RFW-LHN-277 (Trim: E4RFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LHN-277,E4RFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,2,1
E4RFW-LOC (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOC (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOC (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOC (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOC (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOC (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOC (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOC (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOC (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOC (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOC (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOC (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOC (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOC (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOC (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOC (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOC (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOC (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOC (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOC (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOC (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOC (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOC (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOC (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOC (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,2,0
E4RFW-LOC (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,2,0
E4RFW-LOC (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,2,0
E4RFW-LOC (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC,E4RFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOC-277 (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,2,0
E4RFW-LOC-277 (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,2,0
E4RFW-LOC-277 (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,2,0
E4RFW-LOC-277 (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RFW-LOC-277,E4RFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,2,0
E4RFW-LOI (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOI (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOI (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOI (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOI (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOI (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOI (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOI (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOI (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LOI (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LOI (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LOI (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LOI (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOI (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOI (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOI (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOI (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOI (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOI (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOI (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOI (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LOI (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LOI (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LOI (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI,E4RFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LOI (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI,E4RFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,2,0
E4RFW-LOI (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI,E4RFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,2,0
E4RFW-LOI (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI,E4RFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,2,0
E4RFW-LOI (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI,E4RFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LOI-277 (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,2,0
E4RFW-LOI-277 (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,2,0
E4RFW-LOI-277 (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,2,0
E4RFW-LOI-277 (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RFW-LOI-277,E4RFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,2,0
E4RFW-LON (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LON (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LON (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LON (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LON (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-830-B,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,2,2,0
E4RFW-LON (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-830-S,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,3,2,0
E4RFW-LON (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-830-W,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,4,2,0
E4RFW-LON (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,1,2,0
E4RFW-LON (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,2,0
E4RFW-LON (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,2,0
E4RFW-LON (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,2,0
E4RFW-LON (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,2,0
E4RFW-LON (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LON (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LON (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LON (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LON (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-930-B,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,2,2,0
E4RFW-LON (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-930-S,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,3,2,0
E4RFW-LON (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-930-W,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,4,2,0
E4RFW-LON (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,1,2,0
E4RFW-LON (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,2,0
E4RFW-LON (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,2,0
E4RFW-LON (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,2,0
E4RFW-LON (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,2,0
E4RFW-LON (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,2,0
E4RFW-LON (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,2,0
E4RFW-LON (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,2,0
E4RFW-LON (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON,E4RFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-830-B,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-830-S,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-830-W,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-930-B,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-930-S,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-930-W,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,2,0
E4RFW-LON-277 (Trim: E4RFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,2,0
E4RFW-LON-277 (Trim: E4RFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,2,0
E4RFW-LON-277 (Trim: E4RFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,2,0
E4RFW-LON-277 (Trim: E4RFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RFW-LON-277,E4RFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,2,0
E4RLW-LHC (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHC (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHC (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHC (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHC (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHC (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHC (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHC (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHC (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHC (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHC (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHC (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHC (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHC (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHC (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHC (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHC (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHC (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHC (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHC (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHC (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHC (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHC (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHC (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHC (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,1,1
E4RLW-LHC (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,1,1
E4RLW-LHC (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,1,1
E4RLW-LHC (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC,E4RLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHC-277 (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,1,1
E4RLW-LHC-277 (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,1,1
E4RLW-LHC-277 (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,1,1
E4RLW-LHC-277 (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LHC-277,E4RLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,1,1
E4RLW-LHI (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHI (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHI (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHI (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHI (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHI (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHI (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHI (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHI (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHI (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHI (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHI (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHI (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHI (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHI (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHI (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHI (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHI (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHI (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHI (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHI (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHI (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHI (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHI (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI,E4RLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHI (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI,E4RLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,1,1
E4RLW-LHI (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI,E4RLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,1,1
E4RLW-LHI (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI,E4RLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,1,1
E4RLW-LHI (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI,E4RLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHI-277 (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,1,1
E4RLW-LHI-277 (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,1,1
E4RLW-LHI-277 (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,1,1
E4RLW-LHI-277 (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LHI-277,E4RLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,1,1
E4RLW-LHN (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHN (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHN (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHN (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHN (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHN (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHN (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHN (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHN (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,1,1
E4RLW-LHN (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,1,1
E4RLW-LHN (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,1,1
E4RLW-LHN (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,1,1
E4RLW-LHN (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHN (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHN (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHN (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHN (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHN (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHN (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHN (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHN (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,1,1
E4RLW-LHN (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,1,1
E4RLW-LHN (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,1,1
E4RLW-LHN (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,1,1
E4RLW-LHN (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,1,1
E4RLW-LHN (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,1,1
E4RLW-LHN (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,1,1
E4RLW-LHN (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN,E4RLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,1,1
E4RLW-LHN-277 (Trim: E4RLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,1,1
E4RLW-LHN-277 (Trim: E4RLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,1,1
E4RLW-LHN-277 (Trim: E4RLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,1,1
E4RLW-LHN-277 (Trim: E4RLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LHN-277,E4RLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,1,1
E4RLW-LOC (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOC (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOC (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOC (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOC (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOC (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOC (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOC (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOC (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOC (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOC (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOC (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOC (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOC (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOC (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOC (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOC (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOC (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOC (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOC (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOC (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOC (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOC (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOC (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOC (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,1,0
E4RLW-LOC (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,1,0
E4RLW-LOC (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,1,0
E4RLW-LOC (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC,E4RLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOC-277 (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,1,0
E4RLW-LOC-277 (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,1,0
E4RLW-LOC-277 (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,1,0
E4RLW-LOC-277 (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4RLW-LOC-277,E4RLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,1,0
E4RLW-LOI (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOI (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOI (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOI (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOI (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOI (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOI (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOI (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOI (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LOI (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LOI (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LOI (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LOI (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOI (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOI (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOI (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOI (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOI (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOI (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOI (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOI (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LOI (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LOI (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LOI (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI,E4RLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LOI (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI,E4RLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,1,0
E4RLW-LOI (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI,E4RLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,1,0
E4RLW-LOI (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI,E4RLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,1,0
E4RLW-LOI (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI,E4RLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LOI-277 (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,1,0
E4RLW-LOI-277 (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,1,0
E4RLW-LOI-277 (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,1,0
E4RLW-LOI-277 (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4RLW-LOI-277,E4RLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,1,0
E4RLW-LON (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LON (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LON (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LON (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LON (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LON (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LON (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LON (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LON (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,1,0
E4RLW-LON (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,1,0
E4RLW-LON (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,1,0
E4RLW-LON (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,1,0
E4RLW-LON (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LON (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LON (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LON (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LON (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LON (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LON (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LON (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LON (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,1,0
E4RLW-LON (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,1,0
E4RLW-LON (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,1,0
E4RLW-LON (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,1,0
E4RLW-LON (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,1,0
E4RLW-LON (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,1,0
E4RLW-LON (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,1,0
E4RLW-LON (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON,E4RLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,1,0
E4RLW-LON-277 (Trim: E4RLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,1,0
E4RLW-LON-277 (Trim: E4RLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,1,0
E4RLW-LON-277 (Trim: E4RLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,1,0
E4RLW-LON-277 (Trim: E4RLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4RLW-LON-277,E4RLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,1,0
E4SFW-LHC (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHC (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHC (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHC (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHC (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHC (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHC (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHC (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHC (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHC (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHC (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHC (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHC (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHC (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHC (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHC (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHC (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHC (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHC (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHC (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHC (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHC (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHC (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHC (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHC (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,4,1
E4SFW-LHC (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,4,1
E4SFW-LHC (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,4,1
E4SFW-LHC (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC,E4SFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHC-277 (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,4,1
E4SFW-LHC-277 (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,4,1
E4SFW-LHC-277 (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,4,1
E4SFW-LHC-277 (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LHC-277,E4SFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,4,1
E4SFW-LHI (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHI (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHI (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHI (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHI (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHI (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHI (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHI (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHI (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHI (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHI (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHI (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHI (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHI (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHI (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHI (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHI (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHI (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHI (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHI (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHI (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHI (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHI (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHI (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI,E4SFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHI (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI,E4SFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,4,1
E4SFW-LHI (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI,E4SFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,4,1
E4SFW-LHI (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI,E4SFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,4,1
E4SFW-LHI (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI,E4SFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHI-277 (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,4,1
E4SFW-LHI-277 (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,4,1
E4SFW-LHI-277 (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,4,1
E4SFW-LHI-277 (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LHI-277,E4SFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,4,1
E4SFW-LHN (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHN (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHN (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHN (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHN (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-830-B,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,2,4,1
E4SFW-LHN (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-830-S,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,3,4,1
E4SFW-LHN (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-830-W,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,4,4,1
E4SFW-LHN (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-830-Z,31,31 Watts,2343,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,1,4,1
E4SFW-LHN (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,2,4,1
E4SFW-LHN (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,3,4,1
E4SFW-LHN (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,4,4,1
E4SFW-LHN (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,1,1,4,1
E4SFW-LHN (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHN (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHN (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHN (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHN (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-930-B,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,2,4,1
E4SFW-LHN (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-930-S,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,3,4,1
E4SFW-LHN (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-930-W,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,4,4,1
E4SFW-LHN (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-930-Z,31,31 Watts,2000,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,1,4,1
E4SFW-LHN (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,2,4,1
E4SFW-LHN (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,3,4,1
E4SFW-LHN (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,4,4,1
E4SFW-LHN (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,1,1,4,1
E4SFW-LHN (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,2,4,1
E4SFW-LHN (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,3,4,1
E4SFW-LHN (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,4,4,1
E4SFW-LHN (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN,E4SFW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-827-B),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-827-S),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-827-W),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-827-Z),Flanged,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-830-B),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-830-B,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-830-S),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-830-S,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-830-W),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-830-W,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-830-Z),Flanged,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-830-Z,31,31 Watts,2343,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,76,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-835-B),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-835-S),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-835-W),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-835-Z),Flanged,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-927-B),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-927-S),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-927-W),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-927-Z),Flanged,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-930-B),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-930-B,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-930-S),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-930-S,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-930-W),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-930-W,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-930-Z),Flanged,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-930-Z,31,31 Watts,2000,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,64,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-935-B),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-935-S),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-935-W),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-935-Z),Flanged,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,1,1,4,1
E4SFW-LHN-277 (Trim: E4SFW-WD-B),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,2,4,1
E4SFW-LHN-277 (Trim: E4SFW-WD-S),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,3,4,1
E4SFW-LHN-277 (Trim: E4SFW-WD-W),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,4,4,1
E4SFW-LHN-277 (Trim: E4SFW-WD-Z),Flanged,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LHN-277,E4SFW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,1,1,4,1
E4SFW-LOC (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOC (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOC (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOC (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOC (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOC (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOC (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOC (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOC (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOC (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOC (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOC (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOC (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOC (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOC (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOC (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOC (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOC (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOC (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOC (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOC (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOC (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOC (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOC (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOC (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,4,0
E4SFW-LOC (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,4,0
E4SFW-LOC (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,4,0
E4SFW-LOC (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC,E4SFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOC-277 (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,4,0
E4SFW-LOC-277 (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,4,0
E4SFW-LOC-277 (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,4,0
E4SFW-LOC-277 (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SFW-LOC-277,E4SFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,4,0
E4SFW-LOI (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOI (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOI (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOI (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOI (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOI (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOI (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOI (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOI (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LOI (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LOI (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LOI (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LOI (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOI (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOI (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOI (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOI (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOI (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOI (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOI (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOI (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LOI (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LOI (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LOI (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI,E4SFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LOI (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI,E4SFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,4,0
E4SFW-LOI (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI,E4SFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,4,0
E4SFW-LOI (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI,E4SFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,4,0
E4SFW-LOI (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI,E4SFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LOI-277 (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,4,0
E4SFW-LOI-277 (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,4,0
E4SFW-LOI-277 (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,4,0
E4SFW-LOI-277 (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SFW-LOI-277,E4SFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,4,0
E4SFW-LON (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LON (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LON (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LON (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LON (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-830-B,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,2,4,0
E4SFW-LON (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-830-S,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,3,4,0
E4SFW-LON (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-830-W,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,4,4,0
E4SFW-LON (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-830-Z,17,17 Watts,1600,3000,120 Volt,120,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,1,4,0
E4SFW-LON (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,2,4,0
E4SFW-LON (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,3,4,0
E4SFW-LON (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,4,4,0
E4SFW-LON (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,1,1,4,0
E4SFW-LON (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LON (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LON (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LON (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LON (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-930-B,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,2,4,0
E4SFW-LON (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-930-S,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,3,4,0
E4SFW-LON (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-930-W,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,4,4,0
E4SFW-LON (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-930-Z,17,17 Watts,1319,3000,120 Volt,120,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,1,4,0
E4SFW-LON (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,2,4,0
E4SFW-LON (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,3,4,0
E4SFW-LON (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,4,4,0
E4SFW-LON (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,1,1,4,0
E4SFW-LON (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,2,4,0
E4SFW-LON (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,3,4,0
E4SFW-LON (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,4,4,0
E4SFW-LON (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON,E4SFW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-827-B),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-827-S),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-827-W),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-827-Z),Flanged,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-830-B),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-830-B,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-830-S),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-830-S,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-830-W),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-830-W,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-830-Z),Flanged,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-830-Z,17,17 Watts,1600,3000,277 Volt,277,103643585CHI-085 Visual Comfort Group E4SFW-830-W--.ies,84,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-835-B),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-835-S),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-835-W),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-835-Z),Flanged,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-927-B),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-927-S),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-927-W),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-927-Z),Flanged,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-930-B),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-930-B,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-930-S),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-930-S,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-930-W),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-930-W,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-930-Z),Flanged,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-930-Z,17,17 Watts,1319,3000,277 Volt,277,103017649CHI-021 GB E4SFW-LH930N.ies,77,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-935-B),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-935-S),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-935-W),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-935-Z),Flanged,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,1,1,4,0
E4SFW-LON-277 (Trim: E4SFW-WD-B),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,2,4,0
E4SFW-LON-277 (Trim: E4SFW-WD-S),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,3,4,0
E4SFW-LON-277 (Trim: E4SFW-WD-W),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,4,4,0
E4SFW-LON-277 (Trim: E4SFW-WD-Z),Flanged,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SFW-LON-277,E4SFW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,1,1,4,0
E4SLW-LHC (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHC (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHC (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHC (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHC (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHC (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHC (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHC (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHC (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHC (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHC (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHC (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHC (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHC (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHC (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHC (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHC (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHC (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHC (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHC (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHC (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHC (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHC (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHC (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHC (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,3,1
E4SLW-LHC (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,3,1
E4SLW-LHC (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,3,1
E4SLW-LHC (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC,E4SLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHC-277 (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,3,1
E4SLW-LHC-277 (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,3,1
E4SLW-LHC-277 (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,3,1
E4SLW-LHC-277 (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LHC-277,E4SLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,3,1
E4SLW-LHI (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHI (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHI (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHI (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHI (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHI (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHI (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHI (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHI (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHI (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHI (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHI (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHI (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHI (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHI (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHI (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHI (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHI (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHI (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHI (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHI (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHI (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHI (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHI (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI,E4SLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHI (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI,E4SLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,3,1
E4SLW-LHI (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI,E4SLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,3,1
E4SLW-LHI (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI,E4SLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,3,1
E4SLW-LHI (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI,E4SLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHI-277 (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,3,1
E4SLW-LHI-277 (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,3,1
E4SLW-LHI-277 (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,3,1
E4SLW-LHI-277 (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LHI-277,E4SLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,3,1
E4SLW-LHN (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-827-B,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHN (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-827-S,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHN (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-827-W,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHN (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-827-Z,31,31 Watts,2343,2700,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHN (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-830-B,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHN (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-830-S,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHN (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-830-W,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHN (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-830-Z,31,31 Watts,2343,3000,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHN (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-835-B,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,2,3,1
E4SLW-LHN (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-835-S,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,3,3,1
E4SLW-LHN (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-835-W,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,4,3,1
E4SLW-LHN (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-835-Z,31,31 Watts,2343,3500,120 Volt,120,generic.ies,76,0,1,3,1
E4SLW-LHN (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-927-B,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHN (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-927-S,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHN (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-927-W,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHN (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-927-Z,31,31 Watts,2000,2700,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHN (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-930-B,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHN (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-930-S,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHN (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-930-W,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHN (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-930-Z,31,31 Watts,2000,3000,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHN (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-935-B,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,2,3,1
E4SLW-LHN (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-935-S,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,3,3,1
E4SLW-LHN (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-935-W,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,4,3,1
E4SLW-LHN (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-935-Z,31,31 Watts,2000,3500,120 Volt,120,generic.ies,64,0,1,3,1
E4SLW-LHN (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-WD-B,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,2,3,1
E4SLW-LHN (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-WD-S,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,3,3,1
E4SLW-LHN (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-WD-W,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,4,3,1
E4SLW-LHN (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN,E4SLW-WD-Z,31,31 Watts,1875,3000,120 Volt,120,generic.ies,60,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-827-B),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-827-B,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-827-S),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-827-S,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-827-W),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-827-W,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-827-Z),Flangeless,High Output 31W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-827-Z,31,31 Watts,2343,2700,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-830-B),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-830-B,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-830-S),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-830-S,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-830-W),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-830-W,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-830-Z),Flangeless,High Output 31W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-830-Z,31,31 Watts,2343,3000,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-835-B),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-835-B,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-835-S),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-835-S,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-835-W),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-835-W,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-835-Z),Flangeless,High Output 31W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-835-Z,31,31 Watts,2343,3500,277 Volt,277,generic.ies,76,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-927-B),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-927-B,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-927-S),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-927-S,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-927-W),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-927-W,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-927-Z),Flangeless,High Output 31W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-927-Z,31,31 Watts,2000,2700,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-930-B),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-930-B,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-930-S),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-930-S,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-930-W),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-930-W,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-930-Z),Flangeless,High Output 31W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-930-Z,31,31 Watts,2000,3000,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-935-B),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-935-B,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-935-S),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-935-S,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-935-W),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-935-W,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-935-Z),Flangeless,High Output 31W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-935-Z,31,31 Watts,2000,3500,277 Volt,277,generic.ies,64,0,1,3,1
E4SLW-LHN-277 (Trim: E4SLW-WD-B),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-WD-B,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,2,3,1
E4SLW-LHN-277 (Trim: E4SLW-WD-S),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-WD-S,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,3,3,1
E4SLW-LHN-277 (Trim: E4SLW-WD-W),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-WD-W,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,4,3,1
E4SLW-LHN-277 (Trim: E4SLW-WD-Z),Flangeless,High Output 31W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LHN-277,E4SLW-WD-Z,31,31 Watts,1875,3000,277 Volt,277,generic.ies,60,0,1,3,1
E4SLW-LOC (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOC (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOC (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOC (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOC (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOC (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOC (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOC (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOC (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOC (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOC (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOC (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOC (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOC (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOC (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOC (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOC (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOC (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOC (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOC (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOC (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOC (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOC (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOC (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOC (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,3,0
E4SLW-LOC (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,3,0
E4SLW-LOC (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,3,0
E4SLW-LOC (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC,E4SLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOC-277 (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,3,0
E4SLW-LOC-277 (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,3,0
E4SLW-LOC-277 (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,3,0
E4SLW-LOC-277 (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,Chicago Plenum,E4SLW-LOC-277,E4SLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,3,0
E4SLW-LOI (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOI (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOI (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOI (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOI (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOI (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOI (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOI (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOI (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LOI (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LOI (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LOI (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LOI (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOI (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOI (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOI (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOI (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOI (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOI (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOI (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOI (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LOI (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LOI (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LOI (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI,E4SLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LOI (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI,E4SLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,3,0
E4SLW-LOI (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI,E4SLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,3,0
E4SLW-LOI (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI,E4SLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,3,0
E4SLW-LOI (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI,E4SLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LOI-277 (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,3,0
E4SLW-LOI-277 (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,3,0
E4SLW-LOI-277 (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,3,0
E4SLW-LOI-277 (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,IC Airtight,E4SLW-LOI-277,E4SLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,3,0
E4SLW-LON (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-827-B,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LON (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-827-S,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LON (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-827-W,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LON (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-827-Z,17,17 Watts,1600,2700,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LON (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-830-B,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LON (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-830-S,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LON (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-830-W,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LON (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-830-Z,17,17 Watts,1600,3000,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LON (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-835-B,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,2,3,0
E4SLW-LON (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-835-S,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,3,3,0
E4SLW-LON (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-835-W,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,4,3,0
E4SLW-LON (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-835-Z,17,17 Watts,1600,3500,120 Volt,120,generic.ies,84,0,1,3,0
E4SLW-LON (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-927-B,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LON (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-927-S,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LON (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-927-W,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LON (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-927-Z,17,17 Watts,1319,2700,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LON (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-930-B,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LON (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-930-S,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LON (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-930-W,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LON (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-930-Z,17,17 Watts,1319,3000,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LON (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-935-B,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,2,3,0
E4SLW-LON (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-935-S,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,3,3,0
E4SLW-LON (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-935-W,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,4,3,0
E4SLW-LON (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-935-Z,17,17 Watts,1319,3500,120 Volt,120,generic.ies,77,0,1,3,0
E4SLW-LON (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-WD-B,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,2,3,0
E4SLW-LON (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-WD-S,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,3,3,0
E4SLW-LON (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-WD-W,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,4,3,0
E4SLW-LON (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON,E4SLW-WD-Z,17,17 Watts,1000,3000,120 Volt,120,generic.ies,59,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-827-B),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-827-B,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-827-S),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-827-S,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-827-W),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-827-W,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-827-Z),Flangeless,Low Output 17W,80 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-827-Z,17,17 Watts,1600,2700,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-830-B),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-830-B,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-830-S),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-830-S,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-830-W),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-830-W,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-830-Z),Flangeless,Low Output 17W,80 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-830-Z,17,17 Watts,1600,3000,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-835-B),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-835-B,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-835-S),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-835-S,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-835-W),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-835-W,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-835-Z),Flangeless,Low Output 17W,80 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-835-Z,17,17 Watts,1600,3500,277 Volt,277,generic.ies,84,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-927-B),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-927-B,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-927-S),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-927-S,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-927-W),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-927-W,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-927-Z),Flangeless,Low Output 17W,90 CRI 2700K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-927-Z,17,17 Watts,1319,2700,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-930-B),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-930-B,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-930-S),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-930-S,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-930-W),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-930-W,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-930-Z),Flangeless,Low Output 17W,90 CRI 3000K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-930-Z,17,17 Watts,1319,3000,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-935-B),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-935-B,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-935-S),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-935-S,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-935-W),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-935-W,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-935-Z),Flangeless,Low Output 17W,90 CRI 3500K 2-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-935-Z,17,17 Watts,1319,3500,277 Volt,277,generic.ies,77,0,1,3,0
E4SLW-LON-277 (Trim: E4SLW-WD-B),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-WD-B,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,2,3,0
E4SLW-LON-277 (Trim: E4SLW-WD-S),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-WD-S,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,3,3,0
E4SLW-LON-277 (Trim: E4SLW-WD-W),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-WD-W,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,4,3,0
E4SLW-LON-277 (Trim: E4SLW-WD-Z),Flangeless,Low Output 17W,90 CRI 3000-1800K WARM DIM 3-STEP,NON-IC Airtight,E4SLW-LON-277,E4SLW-WD-Z,17,17 Watts,1000,3000,277 Volt,277,generic.ies,59,0,1,3,0
